This page was created by the IDL library routine `mk_html_help2`.

Last modified: Mon Aug 25 17:03:11 2025.

# Directory Listing of Routines

# projects/maven/euv

- MVN_EUV_L0_LOAD
  Load procedure for EUV L0 data. Use for looking at raw EUV data.
- MVN_EUV_L3_LOAD
  Load procedure for the EUV L3 (FISM) daily or minute data
- MVN_EUV_LOAD
  Load procedure for the calibrated EUV irradiances, for

# Routine Descriptions

## MVN_EUV_L0_LOAD

[Next Routine] [List of Routines]

     NAME:
           mvn_euv_l0_load
     PURPOSE:
           Load procedure for EUV L0 data. Use for looking at raw EUV data.
           Use mvn_euv_load instead to load EUV L2 data (calibrated),
           but EUV L2 files are currently about a month behind.
     KEYWORDS:
       trange: specifies the time range
       tplot: plots a time-series of the loaded data
       save: saves tplot files of L0 data for the selected day (only works for 1 day at a time)
       l0: loads data from L0 files instead of tplot files (slow)
       generate: automatically generates daily tplot files for new L0 files
       init: initial date from which to start generating L0 tplot files up to now
     HISTORY:
     VERSION:
      $LastChangedBy: ali $
      $LastChangedDate: 2024-02-27 18:47:50 -0800 (Tue, 27 Feb 2024) $
      $LastChangedRevision: 32462 $
      $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/maven/euv/mvn_euv_l0_load.pro $
    CREATED BY:  ali 20160830
    FILE: mvn_euv_l0_load.pro

(See projects/maven/euv/mvn_euv_l0_load.pro)

## MVN_EUV_L3_LOAD

[Previous Routine] [Next Routine] [List of Routines]

     NAME: mvn_euv_l3_load
     SYNTAX:
           mvn_euv_l3_load,/daily
           or
           mvn_euv_l3_load,/minute
     PURPOSE:
           Load procedure for the EUV L3 (FISM) daily or minute data
     KEYWORDS: daily, minute, ionization_frequency

       Daily:
             loads flare-subtracted data for each day
       Minute:
             loads data with one minute cadence
       ionization_frequency:
             If set to any nonzero value, calculates ionization
             frequencies for CO2, O2, O, CO, N2, Ar according to the
             photoionization cross-sections from the SwRI database:
             http://phidrates.space.swri.edu/ This variable also returns
             a data structure containing all the ionization frequencies

     HISTORY:
     VERSION:
      $LastChangedBy: ali $
      $LastChangedDate: 2017-11-06 12:04:57 -0800 (Mon, 06 Nov 2017) $
      $LastChangedRevision: 24264 $
      $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/maven/euv/mvn_euv_l3_load.pro $
    CREATED BY:  ali 20160401
    FILE: mvn_euv_l3_load.pro

(See projects/maven/euv/mvn_euv_l3_load.pro)

## MVN_EUV_LOAD

[Previous Routine] [List of Routines]

     NAME:
           mvn_euv_load
     SYNTAX:
           mvn_euv_load, trange=trange, /all
     PURPOSE:
           Load procedure for the calibrated EUV irradiances, for
           channels A (17-22 nm), B (0-7 nm), and C (121-122 nm).
     INPUTS
           trange
     OUTPUT:
     KEYWORDS:
     HISTORY:
     VERSION:
      $LastChangedBy: clee $
      $LastChangedDate: 2017-04-27 13:57:56 -0700 (Thu, 27 Apr 2017) $
      $LastChangedRevision: 23232 $
      $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/maven/euv/mvn_euv_load.pro $

    CREATED BY:  Christina O. Lee  02-24-15
    FILE: mvn_euv_load.pro

(See projects/maven/euv/mvn_euv_load.pro)