This page was created by the IDL library routine `mk_html_help2`.

Last modified: Fri Aug 29 03:18:49 2025.

# Directory Listing of Routines

# projects/maven/sta/mvn_sta_gen_tplot_var

- MVN_STA_ETSPEC_DIR
- MVN_STA_ETSPEC_MAGDIR

# Routine Descriptions

## MVN_STA_ETSPEC_DIR

[Next Routine] [List of Routines]

    PROCEDURE:       MVN_STA_ETSPEC_DIR

    PURPOSE:         Makes directional energy-time spectrograms in the
                     specified frame STATIC data.
                     6 tplot variables will be created: +X, -X, +Y, -Y, +Z, and -Z.

    INPUTS:
       APID:         Not necessary, but you can explicitly specify STATIC
                     APID to use. Default is 'd0'.
                     (Note that STATIC data and SPICE kernels need to be
                      loaded beforehand).

    KEYWORDS:        (all keywords are optional.)
       FRAME:        Specifies the frame (Def: 'MSO').

       UNITS:        Specifies the units ('eflux', 'counts', etc.).
                     (Def: 'eflux')

       THLD_THETA:   theta_v > thld_theta => +Z,
                     theta_v < -thld_theta => -Z (Def: 45).

       ATTVEC:       Generates tplot variables showing STATIC XYZ vectors
                     in the specified frame.

       TRANGE:       Time range to compute directional spectra (Def: all).

       MASS:         Specifies mass per charge ranges which you want to use.
                     Default is optimized to be O+ (atomic oxygen ions).

    CREATED BY:      Takuya Hara  on 2014-11-25.

     $LastChangedBy: hara $
     $LastChangedDate: 2015-03-04 06:49:45 -0800 (Wed, 04 Mar 2015) $
     $LastChangedRevision: 17085 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/maven/sta/mvn_sta_gen_tplot_var/mvn_sta_etspec_dir.pro $

(See projects/maven/sta/mvn_sta_gen_tplot_var/mvn_sta_etspec_dir.pro)

## MVN_STA_ETSPEC_MAGDIR

[Previous Routine] [List of Routines]

    PROCEDURE:       MVN_STA_ETSPEC_MAGDIR

    PURPOSE:         Makes directional energy-time spectrogram in the
                     specified pitch angle range from STATIC 4d data.

    INPUTS:          None.
                     (STATIC data should have been loaded and MAG data
                     should have been also inserted into the STATIC
                     common blocks by 'mvn_sta_mag_load' before using
                     this routine.

    KEYWORDS:        (All keywords are optional.)

       APID:         Not necessary, but you can explicitly specify the
                     STATIC APID to use. Default is "d0".

       PITCH:        Specifies the pitch angle range (Def: [0., 30.]).

       UNITS:        Specifies the units ('eflux', 'counts', etc.).
                     (Def: 'eflux')

       TRANGE:       Time range to compute directional spectra (Def: all).

       MASS:         Specifies mass per charge ranges which you want to use.
                     Default is All mass range.

       SUFFIX:       Defines a suffix of the created tplot variable name
                     (Def: e.g., '_ms012-020_pa000-030').

    NOTE:            This routine is based on 'mvn_swia_diretmag' written
                     by Dr. Yuki Harada.

    CREATED BY:      Takuya Hara on 2015-01-21.

     $LastChangedBy: hara $
     $LastChangedDate: 2015-03-04 06:51:10 -0800 (Wed, 04 Mar 2015) $
     $LastChangedRevision: 17086 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/maven/sta/mvn_sta_gen_tplot_var/mvn_sta_etspec_magdir.pro $

(See projects/maven/sta/mvn_sta_gen_tplot_var/mvn_sta_etspec_magdir.pro)