This page was created by the IDL library routine `mk_html_help2`.

Last modified: Thu Sep 11 18:17:40 2025.

# Directory Listing of Routines

# external/IDL_GEOPACK/t89

- KP2IOPT
- T89
- T89_TEST
- TT89

# Routine Descriptions

## KP2IOPT

[Next Routine] [List of Routines]

    Function: kp2iopt

    Purpose: Convert a tplot or array Kp index variable to iopt values suitable for passing to the T89 field
             modeling or tracing routines.

             Input Kp values will be in the range of 0 to 6, and may have a fractional part indicating an increasing or decreasing index.
             For example, 2.33333 represents 2+,  2.66666 represents 3-. iopt output values will be in the range 1 to 7.

    Input: Kp values (e.g. from noaa_load_kp)

    Return value: IOPT values suitable for passing to the GEOPACK T89 tracing and modeling routines.  Represented as double precision floating
            point for compatibility with GEOPACK library calling sequences, but may or may not be rounded to integer values depending
            on whether the kp_plus1 keyword is specified.

    Keywords:
             kp:  (input) A scalar  or array of Kp values, or name of a tplot variable giving the Kp index values

             varname (Required if kp is a tplot variable): A string specifying a tplot position variable.  Output iopt values will be interpolated to the 'varname' times
                      using nearest-neighbor interpolation.

             plus1: (optional)  If specified, overrides the default behavior of rounding iopt to the nearest integer, and
                     instead sets iopt to kp+1, preserving any fractional part.

    Example:

     $LastChangedBy: jwl $
     $LastChangedDate: 2021-07-28 18:16:15 -0700 (Wed, 28 Jul 2021) $
     $LastChangedRevision: 30156 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/external/IDL_GEOPACK/ta15/tomni2bindex.pro $

(See external/IDL_GEOPACK/t89/kp2iopt.pro)

## T89

[Previous Routine] [Next Routine] [List of Routines]

    Function: t89

    Purpose:  generates an array of model magnetic field vectors from
              a monotonic time series and an array of 3-d position
              vectors

    Input:
             tarray: N array representing the time series in seconds utc since 1970
             rgsm_array: Nx3 array representing the position series in earth radii (required to be in GSM coordinates)

    Keywords:
             kp(optional): the requested value of the kp parameter(default: 2)
               kp can also be an array, if it is an array it should be an
               N length array(you should interpolate your values onto the tarray)
               Also kp values passed in can only be integers. any pluses
               or minuses will be ignored, because the Tsyganenko model
               ignores plus and minuses on kp values

             period(optional): the amount of time between recalculations of
                 geodipole tilt and application of a new kp value
                 in seconds,increase this value to decrease run time(default: 600)
                 The center (not the start) of the first period is now aligned with the start time.

             igrf_only(optional): Set this keyword to turn off the t89 component of
               the model and return only the igrf component

             add_tilt:  Increment the default dipole tilt used by the model with
                        a user provided tilt in degrees.  Result will be produced with TSY_DEFAULT_TILT+ADD_TILT
                        Value can be set to an N length array an M length array or a single element array.
                        N is the number of time elements for the data.  M is the number of periods in the time interval.(determined by the period keyword)
                        If single element is provided the same correction will be applied to all periods.
                        If an N length array is provided, the data will be re-sampled to an M length array. Consequently, if
                        the values change quickly, the period may need to be shortened.

             get_tilt: Returns the dipole_tilt parameter used for each period.
                       Returned value has a number of elements equal to the value returned by get_nperiod

             set_tilt: Use alternative dipole_tilt value rather than the geopack tilt.
                       This input can be an M length array, and N length array or a single elemnt.
                       Value can be set to an N length array an M length array or a single element array.
                       N is the number of time elements for the data.  M is the number of periods in the time interval.(determined by the period keyword)
                       If an N length array is provided, the data will be re-sampled to an M length array. Consequently, if
                       the values change quickly, the period may need to be shortened.
                       Notes:
                           1) set_tilt will cause add_tilt to be ignored
                           2) Due to this routine adding IGRF to the returned field, you cannot use set_tilt = 0 and give input
                               position values in SM coordinates; input position values are required to be in GSM coordinates due to the
                               IGRF calculation

             exact_tilt_times (optional):  Set this keyword to avoid grouping similar times (default 10 minutes) and instead
                  recalculate the dipole tilt at each input time

             get_nperiod: Returns the number of periods used for the time interval=  ceil((end_time-start_time)/period)

             geopack_2008 (optional): Set this keyword to use the latest version (2008) of the Geopack
                  library. Version 9.2 of the IDL Geopack DLM is required for this keyword to work.

    Returns:
        an Nx3 length array of field model data (T89 + IGRF) or -1L on failure

    Example:
       mag_array = t89(time_array,pos_array)
       mag_array = t89(time_array,pos_array,kp=5,rlength=10)

    Notes:
      1. Relies on the IDL/Geopack Module provided by Haje Korth JHU/APL
          and N.A. Tsyganenko NASA/GSFC, if the module is not installed
          this function will fail.
      2. Sums the contribution from the internal field model (IGRF) and the
          external field model (t89).
      3. Has a loop with number of iterations = (tarray[n_elements(t_array)]-tarray[0])/period
          This means that as period becomes smaller the amount time of this
          function should take will grow quickly.
      4. Position units are earth radii, be sure to divide your normal
          units by 6371.2 km to convert them.
          6371.2 = the value used in the GEOPACK FORTRAN code for Re

     $LastChangedBy: jwl $
     $LastChangedDate: 2021-12-08 14:28:31 -0800 (Wed, 08 Dec 2021) $
     $LastChangedRevision: 30452 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/external/IDL_GEOPACK/t89/t89.pro $

(See external/IDL_GEOPACK/t89/t89.pro)

## T89_TEST

[Previous Routine] [Next Routine] [List of Routines]

     tt89_test

     Purpose: A few tests to verify that the model and the wrapper
     procedures work correctly

     $LastChangedBy: lphilpott $
     $LastChangedDate: 2012-06-14 11:15:50 -0700 (Thu, 14 Jun 2012) $
     $LastChangedRevision: 10561 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/external/IDL_GEOPACK/t89/t89_test.pro $

(See external/IDL_GEOPACK/t89/t89_test.pro)

## TT89

[Previous Routine] [List of Routines]

    Procedure: tt89

    Purpose:  tplot wrapper for the functional interface to the IDL Geopack
              implementation of the Tsyganenko 89 and IGRF model.

    Input:
              pos_gsm_tvar: the tplot variable storing the position in
                   gsm coordinates(can use standard globbing)

    Keywords:
              kp(optional): the requested value of the kp parameter(default: 2)
                   can also be a tplot variable name if it is a tplot variable name
                   the kp values stored in the variable will be interpolated to match
                   the time grid of the position input values

              period(optional): the amount of time between recalculations of
                   geodipole tilt in seconds(default: 600)  increase this
                   value to decrease run time

              get_nperiod(optional): Return the number of periods used in the time interval

              newname(optional):the name of the output variable.
                   (default: pos_gsm_tvar+'_bt89') This option is ignored if
                   globbing is used.

              error(optional): named variable in which to return the
                   error state of this procedure call. 1 = success, 0 = failure

              igrf_only(optional): Set this keyword to turn off the t89 component of
                   the model and return only the igrf component

              get_tilt(optional):  Set this value to a tplot variable name in which the geodipole tilt for each period will be returned
                   One sample will be returned for each period with time at the center of the period.

              set_tilt(optional): Set this to a tplot variable name or an array of values containing the dipole tilt that should be used.
                   If a tplot input is used it will be interpolated to match the time inputs from the position
                   var. Non-tplot array values must match the number of times in the tplot input for pos_gsm_tvar
                   Notes:
                        1) set_tilt will cause add_tilt to be ignored
                        2) Due to this routine adding IGRF to the returned field, you cannot use set_tilt = 0 and give input
                             position values in SM coordinates; input position values are required to be in GSM coordinates due to the
                             IGRF calculation

              add_tilt(optional): Set this to a tplot variable name or an array of values containing the values to be added to the dipole tilt
                   that should be used for each period. If a tplot input is used it will be interpolated to match the time inputs from the position
                   var. Non-tplot array values must match the number of times in the tplot input for pos_gsm_tvar

             exact_tilt_times (optional):  Set this keyword to avoid grouping similar times (default 10 minutes) and instead
                  recalculate the dipole tilt at each input time

              geopack_2008 (optional): Set this keyword to use the latest version (2008) of the Geopack
                  library. Version 9.2 of the IDL Geopack DLM is required for this keyword to work.

     Output: Stores the result of the field model calculations in tplot variables

     Notes:
            1. Converts from normal gsm to rgsm by dividing vectors by earth's
                radius(6371.2 km) ie inputs should be in km
                6371.2 = the value used in the GEOPACK FORTRAN code for Re
            2. Input must be in GSM coordinates
            3. Haje Korth's IDL/Geopack DLM must be installed for this
            procedure to work

     $LastChangedBy: nikos $
     $LastChangedDate: 2022-08-18 09:29:42 -0700 (Thu, 18 Aug 2022) $
     $LastChangedRevision: 31020 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/external/IDL_GEOPACK/t89/tt89.pro $

(See external/IDL_GEOPACK/t89/tt89.pro)