This page was created by the IDL library routine `mk_html_help2`.

Last modified: Sun Oct 5 03:17:42 2025.

# Directory Listing of Routines

# projects/themis/spedas_plugin

- THEMIS_FILECONFIG
  A widget that allows the user to set some of the fields in the
- THM_UI_GEN_OVERPLOT
  Widget wrapper for spd_ui_overplot used to create THEMIS overview plots in SPEDAS.
- THM_UI_PART_GETSPEC_OPTIONS[1]
  A interface to thm_part_products.pro for creating and loading THEMIS energy/
- THM_UI_PART_GETSPEC_OPTIONS[2]
- THM_UI_PART_PRODUCTS

# Routine Descriptions

## THEMIS_FILECONFIG

[Next Routine] [List of Routines]

    NAME:
     themis_fileconfig

    PURPOSE:
     A widget that allows the user to set some of the fields in the
     !themis system variable: Also allows the user to set the THEMIS
     configuration text file, and save it

    HISTORY:
     17-may-2007, jmm, jimm@ssl.berkeley.edu
     2-jul-2007, jmm, 'Add trailing slash to data directories, if necessary
     5-may-2008, cg, removed text boxes and replaced with radio buttons or
                     pulldowns, fixed reset to default
     10-aug-2011, lphilpott, Added option to set a template to load on startup of gui. Changed layout of widgets
                  slightly to make things line up in both windows and linux.
     24-oct-2013 clr, removed graphic buttons and goes wind and istp code. panel is now tabbed

    $LastChangedBy: jwl $
    $LastChangedDate: 2022-03-01 13:51:02 -0800 (Tue, 01 Mar 2022) $
    $LastChangedRevision: 30635 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spedas_plugin/themis_fileconfig.pro $

(See projects/themis/spedas_plugin/themis_fileconfig.pro)

## THM_UI_GEN_OVERPLOT

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      thm_ui_gen_overplot

    PURPOSE:
      Widget wrapper for spd_ui_overplot used to create THEMIS overview plots in SPEDAS.

    CALLING SEQUENCE:
      See SPEDAS plugin API

    INPUT:
      gui_id:  The id of the main GUI window.
      historyWin:  The history window object.
      oplot_calls:  The number calls to thm_gen_overplot
      callSequence: object that stores sequence of procedure calls that was used to load data
      windowStorage: standard windowStorage object
      windowMenus: standard menu object
      loadedData: standard loadedData object
      drawObject: standard drawObject object

    OUTPUT:
      none

    $LastChangedBy: nikos $
    $LastChangedDate: 2022-03-16 21:14:08 -0700 (Wed, 16 Mar 2022) $
    $LastChangedRevision: 30684 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spedas_plugin/thm_ui_gen_overplot.pro $

(See projects/themis/spedas_plugin/thm_ui_gen_overplot.pro)

## THM_UI_PART_GETSPEC_OPTIONS[1]

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      thm_ui_part_getspec_options

    PURPOSE:
      A interface to thm_part_products.pro for creating and loading THEMIS energy/
      angular particle spectra into the GUI.  Intended to be called from
      SPD_UI_INIT_LOAD_WINDOW.PRO using the SPEDAS load API.

    CALLING SEQUENCE:
      thm_ui_part_getspec_options, tab_id, loadedData, historyWin, statusBar, $
                                   treecopy, trObj, callSequence, $
                                   loadTree=loadTree, $
                                   timeWidget=timeid

    INPUT:
      tab_id:  The widget id of the tab.
      loadedData:  The loadedData object.
      historyWin:  The history window object.
      statusText:  The status bar object for the main Load window.
      treeCopyPtr:  Pointer variable to a copy of the load widget tree.
      trObj:  The GUI timerange object.
      callSequence:  Reference to GUI call sequence object

    OUTPUT:
      loadTree = The Load widget tree.
      timeWidget = The time widget object.

    NOTES:

    HISTORY:
     5-jan-2009, jmm, jimm@ssl.berkeley.edu
     14-jan-2009, jmm, added statusbar object
     15-jan-2009, jmm, added external_state, so that the active data
                       widget on the dproc panel can be updated.
     23-jan-2009, jmm, deletes tplot variables created during processing,
                       correctly updates active data
     13-may-2009, bck, moved code from Data Processing window to Load window
     16-jul-2012, aaf, rewrote error checking on input values to match the
                       behavior of other GUI windows
     ??-sept-2013, aaf, modified to use new spectrogram code
     01-jul-2014, aaf, now conforms to standard SPEDAS load API
     19-mar-2015, aaf, moments, combined data, eclipse corrections, use plugin replay API

    $LastChangedBy: nikos $
    $LastChangedDate: 2019-01-31 09:51:05 -0800 (Thu, 31 Jan 2019) $
    $LastChangedRevision: 26523 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spedas_plugin/thm_ui_part_getspec_options.pro $

(See projects/themis/spedas_plugin/thm_ui_part_getspec_options.pro)

## THM_UI_PART_GETSPEC_OPTIONS[2]

[Previous Routine] [Next Routine] [List of Routines]

     Purpose:
     Helper function to check if strings from user input
     contain valid numbers.
      -returns 1 if widget contains a valid number, 0 otherwise
      -if the input is invalid or out of range then a pop-up
       message will be generated to notify the user

     Arguments:
       state: state data structure
       uname: uname of the widget to check
       namestring: string used to indentify quantity in the
                   error message, e.g "phi min", "maximum energy"

     Keywords (optional):
       min: the minimum valid value for the quantity in question
       max: the maximum valid value for the quantity in question
       value: set to names keyword to return the numeric value
              of the widget

(See projects/themis/spedas_plugin/thm_ui_part_getspec_options.pro)

## THM_UI_PART_PRODUCTS

[Previous Routine] [List of Routines]

    Procedure:
      thm_ui_part_products

    Purpose:
      Wrapper interface between SPEDAS GUI plugin and
      thm_part_products and thm_part_combine.

    Input:
      API Required:
        loaded_data:  SPEDAS loaded data object
        history_window:  SPEDAS history window object
        status_bar:  SPEDAS status bar object

      Unique (options not passed to particle routines):
        load_flags:  flag array denoting which requested probe/datatype/output
                     combinations are to be processed (controls overwrite & replay)

    Output:
      none

    Notes:
      -This routine should comply with the SPEDAS plugin replay API
      -Some particle routines pass keywords to lower level routines through _extra

    $LastChangedBy: aaflores $
    $LastChangedDate: 2015-07-09 19:17:31 -0700 (Thu, 09 Jul 2015) $
    $LastChangedRevision: 18063 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spedas_plugin/thm_ui_part_products.pro $

(See projects/themis/spedas_plugin/thm_ui_part_products.pro)