This page was created by the IDL library routine `mk_html_help2`.

Last modified: Fri Oct 10 18:17:40 2025.

# Directory Listing of Routines

# projects/themis/spin

- CORRECT_DELTA_PHI_TENSOR.PRO
  Apply eclipse delta_phi corrections to L1 MOM tensor quantities.
- CORRECT_DELTA_PHI_VECTOR.PRO
- SEGMENT_INTERP_T
  Performs interpolation on individual elements. (Now a vectorized implementation, accepts multiple inputs)
- SEGMENT_TEST.PRO
  Check a spinmodel segment structure to ensure that the model parameters
- SPINMODEL_FINDSEG_T[1]
  Finds indexes of spin model segments matching each time.
- SPINMODEL_GET_INFO.PRO
  Given a probe string or spinmodel pointer, return information
- SPINMODEL_GET_PTR.PRO
  Returns a pointer to the spin model, specified by a single
- SPINMODEL_INTERP_N.PRO[1]
  Given a spin model and spin count (or array of counts), calculate
- SPINMODEL_INTERP_T.PRO[1]
  Given a spin model and time (or array of times), calculate
- SPINMODEL_POST_PROCESS
- SPINMODEL_RESET.PRO
  Free any data structures associated with the spin model for a
- SPINMODEL_TEST.PRO
  Perform consistency checks on a spin model.
- THM_LOAD_SPIN
- THM_SPINMODEL__DEFINE
  define, construct, and destroy spinmodel objects
- SPINMODEL_FINDSEG_T[2]
  Finds indexes of spin model segments matching each time.
- THM_SPINMODEL::GET_INFO.PRO
  Return information about the valid time range or shadow times given
- SPINMODEL_INTERP_N.PRO[2]
  Given a spin model and spin count (or array of counts), calculate
- SPINMODEL_INTERP_T.PRO[2]
  Given a spin model and time (or array of times), calculate
- THM_SPINMODEL::MAKE_CDF.PRO
  Export the segments data for a spinmodel as tplot variables, then write to a CDF.
- THM_SPINMODEL::MAKE_TPLOT_VARS.PRO
  Export spin model segment attributes as a set of tplot variables
- THM_SPINMODEL::PRINT_SEGMENTS.PRO
  Print the segments contained in a spin model.

# Routine Descriptions

## CORRECT_DELTA_PHI_TENSOR.PRO

[Next Routine] [List of Routines]

     NAME:
        CORRECT_DELTA_PHI_TENSOR.PRO

     PURPOSE:
        Apply eclipse delta_phi corrections to L1 MOM tensor quantities.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
        correct_delta_phi_tensor, tens=mflux, delta_phi=delta_phi

      INPUTS:

      OUTPUTS:

      KEYWORDS:
         tens: An Nx6 input array representing the xx,yy,zz,xy,xz,yz
             components of a 3x3 matrix.  (The other three elements
             are implied by symmetry.)  The data is modified in place.
         delta_phi: An array of delta_phi correction values, in degrees.
             The sample counts of tens and delta_phi must match.

      PROCEDURE:

         For each sample: construct a 3-d rotation matrix corresponding
         to a delta_phi degree counterclockwise rotation about the
         DSL-Z axis.  Construct a 3x3 matrix from the 6-element tensor
         sample.  Apply the rotation by performing matrix multiplication:
         transpose(rotation) # tensor # rotation
         Then strip the redundant terms of the result, yielding a
         modified 6-element representation of the original tensor.

      EXAMPLE:

(See projects/themis/spin/correct_delta_phi_tensor.pro)

## CORRECT_DELTA_PHI_VECTOR.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        CORRECT_DELTA_PHI_VECTOR.PRO

     PURPOSE:

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       correct_delta_phi_vector,tvar=thb_fgs_dsl,delta_phi=delta_phi

      INPUTS:

      OUTPUTS:

      KEYWORDS:
         tvar: name of an input tplot variable containing 3-d vectors in DSL.
            The data will be altered in place.
         x_in, y_in: Input data with X and Y in separate arrays. Output
            goes to variables specified with the x_out and y_out keywords.
         xyz_in: Input data with x,y,z in a single array. Data will be
            altered in place.
         delta_phi: Array of delta_phi values, in degrees.  The sample
            count must match the sample count of the data being transformed.

      PROCEDURE:

     Given a tplot variable name or array(s) of data values (in DSL coordinates),
     and an array of delta_phi values, apply a counter-clockwise rotation of
     delta_phi degrees.  This is used to apply the eclipse delta_phi corrections
     obtained from the spin model, and is intended for correcting spin fits (efs
     and fgs), and (3-vector) particle moments.  Waveform data
     does not require this correction.  Some of the quantities
     from L1 MOM are tensors, and should not be corrected with this
     routine -- see correct_delta_phi_tensor.

(See projects/themis/spin/correct_delta_phi_vector.pro)

## SEGMENT_INTERP_T

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SEGMENT_INTERP_T

     PURPOSE:
        Performs interpolation on individual elements. (Now a vectorized implementation, accepts multiple inputs)

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
      segment_interp_t,segments,t,spincount,t_last,spinphase,spinper,segflag,eclipse_delta_phi

      INPUTS:
        segments: Segment struct from spinmodel
        t: target time array for interpolation(number of elements must match segments)

      OUTPUTS:
        spincount,t_last,spinphase,segflag,eclipse_delta_phi

      KEYWORDS:
        mask=Set to mask value or array of mask value(with same number of elements as segments)

      PROCEDURE:

      EXAMPLE:

    $LastChangedBy: bsadeghi $
    $LastChangedDate: 2012-05-22 10:48:29 -0700 (Tue, 22 May 2012) $
    $LastChangedRevision: 10447 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spin/segment_interp_t.pro $

(See projects/themis/spin/segment_interp_t.pro)

## SEGMENT_TEST.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SEGMENT_TEST.PRO

     PURPOSE:
        Check a spinmodel segment structure to ensure that the model parameters
        b and c are consistent with the start and end times and
        spin counts

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       segment_test,probe,segment,result

      INPUTS:
        probe: A single character probe letter (only used in output messages).
        segment: A spinmodel_segment structure.

      OUTPUTS:
        result: 0 for failure, 1 for success

      KEYWORDS:
        None.

      PROCEDURE:
        Calls segment_interp_t to get spin count and spin phase at
           segment start/end times.
        Calls segment_interp_n to get sun pulse times of segment
           start/end counts.
        Cross check results of segment_interp_t and segment_interp_n,
           verifying that interp_t and interp_n results are consistent
           within modest tolerances (100 usec for times, 0.1 deg for
           phase angles).
        Check maxgap field against 4-hour threshold; large gaps are
           likely a result of missing data.

      EXAMPLE:
        mptr=spinmodel_get_ptr('a')
        sptr=(*mptr).segs_ptr
        segment_test,'a',(*sptr)[0],result

    Written by: Jim Lewis (jwl@ssl.berkeley.edu)
    Change Date: 2007-10-08

(See projects/themis/spin/segment_test.pro)

## SPINMODEL_FINDSEG_T[1]

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_FINDSEG_T

     PURPOSE:
        Finds indexes of spin model segments matching each time.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
      spinmodel_findseg_t,mptr,t

      INPUTS:
        mptr: pointer to spin model
        t: array of times to which model segments will be matched

      RETURNS:
        an array of matching indexes.  Throws error using 'message' routine on failure.

      PROCEDURE:

      EXAMPLE:

    $LastChangedBy: pcruce $
    $LastChangedDate: 2010-10-25 13:18:23 -0700 (Mon, 25 Oct 2010) $
    $LastChangedRevision: 7885 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spin/spinmodel_findseg_t.pro $

(See projects/themis/spin/spinmodel_findseg_t.pro)

## SPINMODEL_FINDSEG_T[2]

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_FINDSEG_T

     PURPOSE:
        Finds indexes of spin model segments matching each time.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
      model->spinmodel_findseg_t,t

      INPUTS:
        model: spin model, reference to object of type 'thm_spinmodel'
        t: array of times to which model segments will be matched

      RETURNS:
        an array of matching indexes.  Throws error using 'message' routine on failure.

      PROCEDURE:

      EXAMPLE:

    $LastChangedBy: jwl $
    $LastChangedDate: 2011-05-09 11:16:41 -0700 (Mon, 09 May 2011) $
    $LastChangedRevision: 8651 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spin/thm_spinmodel__findseg_t.pro $

(See projects/themis/spin/thm_spinmodel__findseg_t.pro)

## SPINMODEL_GET_INFO.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_GET_INFO.PRO

     PURPOSE:
        Given a probe string or spinmodel pointer, return information
        about the valid time range or shadow times.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel_get_info,model=modelptr,min_shadow_duration=min_shadow_duration,$
          shadow_count=shadow_count, $
          shadow_start=shadow_start,shadow_end=shadow_end,$
          start_time=start_time, end_time=end_time

      INPUTS:
        Model: pointer to s spinmodel structure
        Probe: a string identifying the probe.
           The caller must specify either a model pointer or probe string.
        min_shadow_duration: Optional parameter specifying the minimum
           gap between BAU sun sensor crossing times to be considered a shadow
           interval. Defaults to 60.0 sec.

      OUTPUTS: (all optional)
        shadow_count: Number of shadow intervals found.
        shadow_start: Double precision array of shadow start times.
        shadow_end: Double precision array of shadow end times.
        start_time: Double precision scalar indicating start time
           of loaded spinmodel data
        end_time: Double precision scalar indicating end time of
           loaded spinmodel data

      PROCEDURE:
         Shadow intervals consist of spinmodel segments where the
           "maxgap" parameter exceeds the min_shadow_duration threshold.
         Start time is the start time of the first segment.
         End time is the end time of the last segment.
         If no spinmodel data is loaded for the requested probe,
         start_time = end_time = 0.0D.
         If no shadows are found, shadow_count is set to zero and
         no start/end times are returned.

      EXAMPLE:
         timespan,'2007-03-23',1,/days
         thm_load_state,probe='a',/get_support_data

         spinmodel_get_info,probe='a',shadow_count=shadow_count,$
           shadow_start=shadow_start, shadow_end=shadow_end,$
           start_time=start_time,end_time=end_time

(See projects/themis/spin/spinmodel_get_info.pro)

## SPINMODEL_GET_PTR.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_GET_PTR.PRO

     PURPOSE:
       Returns a pointer to the spin model, specified by a single
       letter probe designation ('a' through 'f').  This is to avoid
       having to define the spinmodel common block all over the place.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       model_ptr=spinmodel_get_ptr('a')

      INPUTS:
        probe: A scalar character, one of 'a' through 'f', specifying which model
           pointer to return.

      OUTPUTS:
        model_ptr: The return value is a pointer to the specified spin model,
           suitable for passing to the other spinmodel manipulation routines.

      KEYWORDS:
        /QUIET : Do not print message if a spin model has not yet been loaded (prevents confusing warning in thm_autoload_support)

      PROCEDURE:
        Test probe argument for validity; return appropriate value from
        the spinmodel_common block.

      EXAMPLE:
         model_ptr=spinmodel_get_ptr('a')
         spinmodel_test,model_ptr

    Written by: Jim Lewis (jwl@ssl.berkeley.edu)
    Change Date: 2007-10-08

(See projects/themis/spin/spinmodel_get_ptr.pro)

## SPINMODEL_INTERP_N.PRO[1]

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_INTERP_N.PRO

     PURPOSE:
        Given a spin model and spin count  (or array of counts), calculate
        the sun pulse time and spin period at each input count.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel_interp_n,model=modelptr,count=input_counts,$
          time=output_times, spinper=output_spinper

      INPUTS:
        Model: pointer to a spinmodel structure
        Count: A long integer (or long integer array) specifying the spin
          count to use.  If the input is a scalar, all outputs
          will be scalars; otherwise, all outputs are arrays having
          the same size as the input counts.

      OUTPUTS:
        spinper: Optional keyword parameter to receive spin period values.
        time: Optional keyword parameter to receive sun pulse time
           of each input count.

      KEYWORDS:

      /MODEL: Required input keyword argument, specifying a pointer to a
          spinmodel structure.
      /COUNT: Required input keyword argument specifying a time or array of times.
      /SPINPER: Optional keyword argument to receive spin period values.
      /TIME:  Optional keyword argument to receive sun pulse times.

      PROCEDURE:
         Find the spinmodel segment containing the input spin count.
         Invert phi(t) function to find time corresponding to this count.
         Use b and c segment parameters to determine the spin period
           at the sunpulse time.

      EXAMPLE:
      ; Retrieve first 100 sun pulse times included in model for THA:
      modelptr=spinmodel_get_ptr('a')
      spinmodel_interp_n,model=modelptr,count=lindgen(100),time=output_times

(See projects/themis/spin/spinmodel_interp_n.pro)

## SPINMODEL_INTERP_N.PRO[2]

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_INTERP_N.PRO

     PURPOSE:
        Given a spin model and spin count  (or array of counts), calculate
        the sun pulse time and spin period at each input count.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel->interp_n,count=input_counts,$
          time=output_times, spinper=output_spinper

      INPUTS:
        Count: A long integer (or long integer array) specifying the spin
          count to use.  If the input is a scalar, all outputs
          will be scalars; otherwise, all outputs are arrays having
          the same size as the input counts.

      OUTPUTS:
        spinper: Optional keyword parameter to receive spin period values.
        time: Optional keyword parameter to receive sun pulse time
           of each input count.

      KEYWORDS:

      /COUNT: Required input keyword argument specifying a time or array of times.
      /SPINPER: Optional keyword argument to receive spin period values.
      /TIME:  Optional keyword argument to receive sun pulse times.

      PROCEDURE:
         Find the spinmodel segment containing the input spin count.
         Invert phi(t) function to find time corresponding to this count.
         Use b and c segment parameters to determine the spin period
           at the sunpulse time.

      EXAMPLE:
      ; Retrieve first 100 sun pulse times included in model for THA:
      modelptr=spinmodel_get_ptr('a')
      spinmodel_interp_n,model=modelptr,count=lindgen(100),time=output_times

(See projects/themis/spin/thm_spinmodel__interp_n.pro)

## SPINMODEL_INTERP_T.PRO[1]

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_INTERP_T.PRO

     PURPOSE:
        Given a spin model and time (or array of times), calculate
        the spin count, spin phase, spin period, and time of last sun pulse
        for each input time.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel_interp_t,model=modelptr,time=input_times,$
          spincount=output_spincount, spinper=output_spinper,$
          t_last=output_sun_pulse_times, eclipse_delta_phi=delta_phi

      INPUTS:
        Model: pointer to s spinmodel structure
        Time: A double precision scalar or array specifying the input times.
          If the input is a scalar, all outputs will be scalars; otherwise,
          all outputs are arrays having the same size as the input times.

      OUTPUTS:
        spinper: Optional keyword parameter to receive spin period values.
        tlast: Optional keyword parameter to receive sun pulse time
           immediately preceding each input time.
        spincount: Optional keyword parameter to receive count of spins
           since the start of the model.
        spinphase: Optional keyword parameter to receive the spin phase
           (ranging from 0.0 to 360.0 degrees) at each input time.
        eclipse_delta_phi: Optional keyword parameter to receive
           deviation (degrees) between the IDPU's spin model and
           the sunpulse+fgm spin model. Zero in sunlight, non-zero
           if in eclipse AND FGM "synthetic" sunpulses were used
           when the spinmodel was created during L0->L1 processing.

      KEYWORDS:

      /MODEL: Required input keyword argument, specifying a pointer to a
          spinmodel structure.
      /TIME: Required input keyword argument specifying a time or array of times.
      /SPINPER: Optional keyword argument to receive spin period values.
      /T_LAST:  Optional keyword argument to receive sun pulse times
      /SPINCOUNT:  Optional keyword argument to receive spin counts
      /SPINPHASE:  Optional keyword argument to receive spin phase

      PROCEDURE:
         Find the spinmodel segment containing the input time.
         Use b and c segment parameters to determine the spin period,
           spin phase, and spin count at each input time
         Invert phi(t) function to find sun pulse time immediately preceding
           each input time.

      EXAMPLE:

      ; Assume 'input_times' and 'input_spinphase' already exist as a
      ; IDL variables -- perhaps obtained from thm_load_state.
      ;
      ; Get a pointer to the spin model for probe A
      modelptr=spinmodel_get_ptr('a')

      ; Calculate spin phase at each time from spin model

      spinmodel_interp_t,model=modelptr,time=input_times,spinphase=output_spinphase

      ; Calculate spinphase differences between spin model and state
      phi_diff=output_spinphase-input_spinphase

      ; Fix wraparounds

      i=where(phi_diff GT 180.0D)
      i2=where(phi_diff LT -180.0D)
      phi_diff[i] = phi_diff[i] - 360.0D
      phi_diff[i2] = phi_diff[i2] + 360.0D

      Plot results

      plot,input_times,phi_diff

(See projects/themis/spin/spinmodel_interp_t.pro)

## SPINMODEL_INTERP_T.PRO[2]

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_INTERP_T.PRO

     PURPOSE:
        Given a spin model and time (or array of times), calculate
        the spin count, spin phase, spin period, and time of last sun pulse
        for each input time.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel->interp_t,time=input_times,$
          spincount=output_spincount, spinper=output_spinper,$
          t_last=output_sun_pulse_times, segflag=output_segflag, eclipse_delta_phi=delta_phi

      INPUTS:
        Time: A double precision scalar or array specifying the input times.
          If the input is a scalar, all outputs will be scalars; otherwise,
          all outputs are arrays having the same size as the input times.

      OUTPUTS:
        spinper: Optional keyword parameter to receive spin period values.
        tlast: Optional keyword parameter to receive sun pulse time
           immediately preceding each input time.
        spincount: Optional keyword parameter to receive count of spins
           since the start of the model.
        spinphase: Optional keyword parameter to receive the spin phase
           (ranging from 0.0 to 360.0 degrees) at each input time.
        eclipse_delta_phi: Optional keyword parameter to receive
           deviation (degrees) between the IDPU's spin model and
           the sunpulse+fgm spin model. Zero in sunlight, non-zero
           if in eclipse AND FGM "synthetic" sunpulses were used
           when the spinmodel was created during L0->L1 processing.

      KEYWORDS:

      /TIME: Required input keyword argument specifying a time or array of times.
      /SPINPER: Optional keyword argument to receive spin period values.
      /T_LAST:  Optional keyword argument to receive sun pulse times
      /SPINCOUNT:  Optional keyword argument to receive spin counts
      /SPINPHASE:  Optional keyword argument to receive spin phase

      PROCEDURE:
         Find the spinmodel segment containing the input time.
         Use b and c segment parameters to determine the spin period,
           spin phase, and spin count at each input time
         Invert phi(t) function to find sun pulse time immediately preceding
           each input time.

      EXAMPLE:

      ; Assume 'input_times' and 'input_spinphase' already exist as a
      ; IDL variables -- perhaps obtained from thm_load_state.
      ;
      ; Get a pointer to the spin model for probe A
      modelptr=spinmodel_get_ptr('a')

      ; Calculate spin phase at each time from spin model

      model->interp_t,time=input_times,spinphase=output_spinphase

      ; Calculate spinphase differences between spin model and state
      phi_diff=output_spinphase-input_spinphase

      ; Fix wraparounds

      i=where(phi_diff GT 180.0D)
      i2=where(phi_diff LT -180.0D)
      phi_diff[i] = phi_diff[i] - 360.0D
      phi_diff[i2] = phi_diff[i2] + 360.0D

      Plot results

      plot,input_times,phi_diff

(See projects/themis/spin/thm_spinmodel__interp_t.pro)

## SPINMODEL_POST_PROCESS

[Previous Routine] [Next Routine] [List of Routines]

     Function: spinmodel_post_process

     Purpose: Performs post-load corrections on spinmodel data.

     Notes: Somewhat finicky about data requirements.  Will throw an error that
      causes interpreter to halt unless the error is explicitly caught.  Error's
      will be returned in the SPINMODEL_POST_PROCESS message block.

      If you find execution halted here and you aren't sure why, it is probably
      because the state support data was not loaded.
      This occurs most commonly because
      1. there is no data available on this day, or
      2. because of internet connection issues,
      3. because the !themis.no_download flag is on.

     $LastChangedBy: bsadeghi $
     $LastChangedDate: 2012-05-22 10:48:29 -0700 (Tue, 22 May 2012) $
     $LastChangedRevision: 10447 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/themis/spin/spinmodel_post_process.pro $

(See projects/themis/spin/spinmodel_post_process.pro)

## SPINMODEL_RESET.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_RESET.PRO

     PURPOSE:
        Free any data structures associated with the spin model for a
        given probe or set of probes, and null out the spin model
        pointer to prevent stale, previously loaded data from being
        used erroneously.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel_reset,probe='a'
       spinmodel_reset,probe='a b c'
       spinmodel_reset,probe=['a','b','c']
       spinmodel_reset,probe='*'
       spinmodel_reset,probe='all'

      INPUTS:
        None.

      OUTPUTS:
        None.

      KEYWORDS:
        PROBE  Specifies which probe or probes to reset.

      PROCEDURE:
        Parse value of PROBE keyword to see which models to reset;
        for any specified model with existing data, free the data
        and set the spinmodel pointer in the common block to null.

      EXAMPLE:

    Written by: Jim Lewis (jwl@ssl.berkeley.edu)

(See projects/themis/spin/spinmodel_reset.pro)

## SPINMODEL_TEST.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        SPINMODEL_TEST.PRO

     PURPOSE:
       Perform consistency checks on a spin model.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel_test,model_ptr

      INPUTS:
        model_ptr: A pointer to a spinmodel structure, obtained from the
        spinmodel_common block or the spinmodel_get_ptr() function.
        This input must be a scalar.

      OUTPUTS:
        Prints "PASS"/"FAIL" messages depending on outcome of tests.

      KEYWORDS:
        None.

      PROCEDURE:
        Validate model_ptr input argument.
        Compare spin model capacity to actual number of segments.
        Validate pointer to model segments.
        Call segment_test on each model segment, check for any failures.
        Examine boundaries of adjacent segments, making sure time and
           spin_number endpoints are identical across each pair.
        Exercise spinmodel_interp_n by retrieving modeled sun pulse
           times by spin number.
        Exercise spinmodel_interp_t by recalculating the spin count
           and spin phase at each modeled sun pulse time.
        Cross check results of spinmodel_interp_n and spinmodel_interp_t
           to verify that the expected values are produced within
           modest tolerances (allowable phase error .01 deg at each
           modeled sun pulse time).

      EXAMPLE:
         model_ptr=spinmodel_get_ptr('a')
         spinmodel_test,model_ptr

    Written by: Jim Lewis (jwl@ssl.berkeley.edu)
    Change Date: 2007-10-08

(See projects/themis/spin/spinmodel_test.pro)

## THM_LOAD_SPIN

[Previous Routine] [Next Routine] [List of Routines]

    Procedure: THM_LOAD_SPIN

    Purpose:  Loads THEMIS spin model parameters, performs some post-processing
     of data loaded from the SPIN CDFs, and stashes the resulting spin model
     in a common block.

    keywords:
      probe = Probe name. The default is 'all', i.e., load all available probes.
              This can be an array of strings, e.g., ['a', 'b'] or a
              single string delimited by spaces, e.g., 'a b'
              Flatsat data (probe 'f') is not returned unless explicitly
              mentioned.
      datatype = The type of data to be loaded, can be an array of strings
              or single string separate by spaces.  The default is 'all'
      TRANGE= (Optional) Time range of interest  (2 element array), if
              this is not set, the default is to prompt the user. Note
              that if the input time range is not a full day, a full
              day's data is loaded
      level = the level of the data, the default is 'l1', or level-1
              data. A string (e.g., 'l2') or an integer can be used. 'all'
              can be passed in also, to get all levels.
      CDF_DATA: named variable in which to return cdf data structure: only works
              for a single spacecraft and datafile name.
      VARNAMES: names of variables to load from cdf: default is all.
      /GET_SUPPORT_DATA: load support_data variables as well as data variables
                          into tplot variables.
      /DOWNLOADONLY: download file but don't read it.
      /valid_names, if set, then this routine will return the valid probe, datatype
              and/or level options in named variables supplied as
              arguments to the corresponding keywords.
      files   named varible for output of pathnames of local files.
      /VERBOSE  set to output some useful info
    Example:
       thm_load_spin,probe=['a','b']

    Written by: Jim Lewis (jwl@ssl.berkeley.edu)
    Change Date: 2007-10-08

(See projects/themis/spin/thm_load_spin.pro)

## THM_SPINMODEL::GET_INFO.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        THM_SPINMODEL::GET_INFO.PRO

     PURPOSE:
        Return information about the valid time range or shadow times given
        a spinmodel object reference.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel->get_info,min_shadow_duration=min_shadow_duration,$
          shadow_count=shadow_count, $
          shadow_start=shadow_start,shadow_end=shadow_end,$
          start_time=start_time, end_time=end_time

      INPUTS:
        min_shadow_duration: Optional parameter specifying the minimum
           gap between BAU sun sensor crossing times to be considered a shadow
           interval. Defaults to 60.0 sec.

      OUTPUTS: (all optional)
        shadow_count: Number of shadow intervals found.
        shadow_start: Double precision array of shadow start times.
        shadow_end: Double precision array of shadow end times.
        start_time: Double precision scalar indicating start time
           of loaded spinmodel data
        end_time: Double precision scalar indicating end time of
           loaded spinmodel data

      PROCEDURE:
         Shadow intervals consist of spinmodel segments where the
           "maxgap" parameter exceeds the min_shadow_duration threshold.
         Start time is the start time of the first segment.
         End time is the end time of the last segment.
         If no spinmodel data is loaded for the requested probe,
         start_time = end_time = 0.0D.
         If no shadows are found, shadow_count is set to zero and
         no start/end times are returned.

      EXAMPLE:
         timespan,'2007-03-23',1,/days
         thm_load_state,probe='a',/get_support_data

         spinmodel_get_info,probe='a',shadow_count=shadow_count,$
           shadow_start=shadow_start, shadow_end=shadow_end,$
           start_time=start_time,end_time=end_time

(See projects/themis/spin/thm_spinmodel__get_info.pro)

## THM_SPINMODEL::MAKE_CDF.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        THM_SPINMODEL::MAKE_CDF.PRO

     PURPOSE:
         Export the segments data for a spinmodel as tplot variables, then write to a CDF.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       smp = spinmodel_get_ptr('a',use_eclipse_corrections=2)

      INPUTS:
        prefix: A string to be prepended to segment attribute names to form tplot variables
        cdf_filename: The filename of the CDF to be produced.

      OUTPUTS: (all optional)
        None

      EXAMPLE:
         timespan,'2007-03-23',1,/days
         thm_load_state,probe='a',/get_support_data

         smp = spinmodel_get_ptr('a',use_eclipse_corrections=2)
         smp->make_cdf,prefix='tha_corr2_',cdf_filename='tha_corr2.cdf'

(See projects/themis/spin/thm_spinmodel__make_cdf.pro)

## THM_SPINMODEL::MAKE_TPLOT_VARS.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        THM_SPINMODEL::MAKE_TPLOT_VARS.PRO

     PURPOSE:
        Export spin model segment attributes as a set of tplot variables

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel->make_tplot_vars,prefix=prefix

      INPUTS:
        prefix:  A string to be prepended to each segment attribute to form tplot variable names.

      OUTPUTS:
        None

      EXAMPLE:
         timespan,'2007-03-23',1,/days
         thm_load_state,probe='a',/get_support_data

         smp = spinmodel_get_ptr('a',use_eclipse_corrections=2)
         smp->make_tplot_vars,prefix='tha_corr2_'

(See projects/themis/spin/thm_spinmodel__make_tplot_vars.pro)

## THM_SPINMODEL::PRINT_SEGMENTS.PRO

[Previous Routine] [Next Routine] [List of Routines]

     NAME:
        THM_SPINMODEL::PRINT_SEGMENTS.PRO

     PURPOSE:
        Print the segments contained in a spin model.

     CATEGORY:
       TDAS

     CALLING SEQUENCE:
       spinmodel->print_segments

      INPUTS:
        None

      OUTPUTS:
        None

      EXAMPLE:
         timespan,'2007-03-23',1,/days
         thm_load_state,probe='a',/get_support_data

         smp=spinmodel_get_ptr('a',use_eclipse_corrections=2)
         smp->print_segments

(See projects/themis/spin/thm_spinmodel__print_segments.pro)

## THM_SPINMODEL__DEFINE

[Previous Routine] [List of Routines]

    NAME:
     thm_spinmodel__define
    PURPOSE:
     define, construct, and destroy spinmodel objects

(See projects/themis/spin/thm_spinmodel__define.pro)