;=============================
; Bentpipe is a FPI Emergency parameters to be used when DFG/AFG not available.
;=============================

;-------------
; AE index
;-------------
thg_idx_ae

;-----------------
; Magnetic Field
;-----------------
mms*_fpi_bentPipeB_DBCS;.... Bx, By, Bz 
mms*_fpi_bentPipeB_DBCS_z;.... Bz
mms*_fpi_bentPipeB_Norm;... |B|

;---------------------
; S/C Potential
;---------------------
mms*_edp_scpot_fast_sitl; SC-potential

;----------------------------------
; Density, Velocity
;----------------------------------
mms*_fpi_density; ... FPI
mms*_fpi_ion_vel_dbcs;... FPI

;--------------------
; Spectrograms
;--------------------
mms*_epd_eis_extof_proton_flux_omni_spin
mms*_fpi_ions ;.............. FPI
mms*_hpca_oplus_omni_flux
mms*_epd_feeps_srvy_sitl_electron_intensity_omni_spin
mms*_fpi_electrons;........... FPI

;--------------------
; Waves
;--------------------
mms*_edp_fast_dce_sitl;....... E-field waveform
mms*_edp_hfesp_srvy_l2;........ E-field spectrum
mms*_dsp_bpsd_omni_fast_l2;.... B-field spectrum

;--------------------
; SITL
;--------------------
mms*_sroi; Science ROIs
mms_soca_mdq; MDQ
mms_soca_fomstr; FOM (ABS) (Automated Burst Selection generated by SOC Automatic Algorithm)
mms_stlm_fomstr; FOM (current) (being modified by a SITL)
mms_stlm_fomstr_copy; FOM (temporary selections for comparison with FOM (current))
;mms_soca_bakstr; BAK (SITL) (Latest BDM status after SITL modification)
mms_stlm_bakstr; BAK (current) (being modified by a super-SITL)
