This page was created by the IDL library routine `mk_html_help2`.

Last modified: Wed Nov 5 03:16:59 2025.

# Directory Listing of Routines

# external/IDL_GEOPACK/t04s

- T04S
- T04S_TEST
- TT04S

# Routine Descriptions

## T04S

[Next Routine] [List of Routines]

    Function: t04s

    Purpose:  generates an array of model magnetic field vectors from
              a monotonic time series and an array of 3-d position
              vectors

    Input:
             tarray: N array representing the time series in seconds utc since 1970
             rgsm_array: Nx3 array representing the position series in
                 earth radii (required to be in GSM coordinates)
             The following arguments can either be N length arrays or
             single values
             pdyn_array: Solar wind pressure (nanoPascals)
             dsti_array: DST index(nanoTeslas)
             yimf_array: y component of the interplanetary magnetic field
             zimf_array: z component of the interplanetary magnetic field
             w1_array:  index represents a time integral over a storm
             w2_array:  index represents a time integral over a storm
             w3_array:  index represents a time integral over a storm
             w4_array:  index represents a time integral over a storm
             w5_array:  index represents a time integral over a storm
             w6_array:  index represents a time integral over a storm

    Keywords:
             period(optional): the amount of time between recalculations of
                 geodipole tilt in seconds(default: 60)
                 increase this value to decrease run time

             add_tilt:  Increment the default dipole tilt used by the model with
                        a user provided tilt in degrees.  Result will be produced with TSY_DEFAULT_TILT+ADD_TILT
                        Value can be set to an N length array an M length array or a single element array.
                        N is the number of time elements for the data.  M is the number of periods in the time interval.(determined by the period keyword)
                        If single element is provided the same correction will be applied to all periods.
                        If an N length array is provided, the data will be re-sampled to an M length array. Consequently, if
                        the values change quickly, the period may need to be shortened.

             get_tilt: Returns the dipole_tilt parameter used for each period.
                       Returned value has a number of elements equal to the value returned by get_nperiod

             set_tilt: Alternative dipole_tilt value rather than the geopack tilt.
                       This input can be an M length array, and N length array or a single elemnt.
                       Value can be set to an N length array an M length array or a single element array.
                       N is the number of time elements for the data.  M is the number of periods in the time interval.(determined by the period keyword)
                       If an N length array is provided, the data will be re-sampled to an M length array. Consequently, if
                       the values change quickly, the period may need to be shortened.
                       Notes:
                           1) set_tilt will cause add_tilt to be ignored
                           2) Due to this routine adding IGRF to the returned field, you cannot use set_tilt = 0 and give input
                               position values in SM coordinates; input position values are required to be in GSM coordinates due to the
                               IGRF calculation

             exact_tilt_times (optional):  Set this keyword to avoid grouping similar times (default 10 minutes) and instead
                  recalculate the dipole tilt at each input time

             get_nperiod: Returns the number of periods used for the time interval=  ceil((end_time-start_time)/period)

             geopack_2008 (optional): Set this keyword to use the latest version (2008) of the Geopack
                  library. Version 9.2 of the IDL Geopack DLM is required for this keyword to work.

             IOPGEN (optional): General option flag to pass to geopack_ts04. From Tsyganenko's Fortran:
                                      IOPGEN=0 - CALCULATE TOTAL FIELD
                                      IOPGEN=1 - DIPOLE SHIELDING ONLY
                                      IOPGEN=2 - TAIL FIELD ONLY
                                      IOPGEN=3 - BIRKELAND FIELD ONLY
                                      IOPGEN=4 - RING CURRENT FIELD ONLY
                                      IOPGEN=5 - INTERCONNECTION FIELD ONLY

             IOPT (optional)
             -  TAIL FIELD FLAG:       IOPT=0  -  BOTH MODES
                                       IOPT=1  -  MODE 1 ONLY
                                       IOPT=2  -  MODE 2 ONLY

             IOPB (optional)
             -  BIRKELAND FIELD FLAG: IOPB=0  -  ALL 4 TERMS
                                      IOPB=1  -  REGION 1, MODES 1 AND 2
                                      IOPB=2  -  REGION 2, MODES 1 AND 2

             IOPR (optional)
             -  RING CURRENT FLAG:    IOPR=0  -  BOTH SRC AND PRC
                                      IOPR=1  -  SRC ONLY
                                      IOPR=2  -  PRC ONLY

    Returns: an Nx3 length array of field model data (TS04 + IGRF) or -1L on failure

    Example:
       mag_array = t04s(time_array,pos_array,pdyn_array,dsti_array,yimf_array,zimf_array,w1_array,w2_array,w3_array,w4_array,w5_array,w6_array)
       mag_array = t04s(time_array,pos_array,pdyn_array,dsti_array,yimf_array,zimf_array,w1_array,w2_array,w3_array,w4_array,w5_array,w6_array,period=10)

    Notes:
      1. Relies on the IDL/Geopack Module provided by Haje Korth JHU/APL
          and N.A. Tsyganenko NASA/GSFC, if the module is not installed
          this function will fail.
      2. Sums the contribution from the internal field model and the
          external field model.
      3. Has a loop with number of iterations = (tarray[n_elements(t_array)]-tarray[0])/period
          This means that as period becomes smaller the amount time of this
          function should take will grow quickly.
      4. Position units are in earth radii, be sure to divide your normal
          units by 6371.2 km to convert them.
          6371.2 = the value used in the GEOPACK FORTRAN code for Re
      5.Find more documentation on the inner workings of the model,
          any gotchas, and the meaning of the arguments at:
          http://geo.phys.spbu.ru/~tsyganenko/modeling.html
          -or-
          http://ampere.jhuapl.edu/code/idl_geopack.html
      6. Definition of W1-W6 can be found at:
          N. A. Tsyganenko and M. I. Sitnov, Modeling the dynamics of the
          inner magnetosphere during strong geomagnetic storms, J. Geophys.
          Res., v. 110 (A3), A03208, doi: 10.1029/2004JA010798, 2005
      7. The dipole tilt calculation periods are now set so that the center (not the start) of the first period is
          aligned with the first timestamp.  JWL 2021-03-22

     $LastChangedBy: jwl $
     $LastChangedDate: 2021-06-24 16:12:40 -0700 (Thu, 24 Jun 2021) $
     $LastChangedRevision: 30083 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/external/IDL_GEOPACK/t04s/t04s.pro $

(See external/IDL_GEOPACK/t04s/t04s.pro)

## T04S_TEST

[Previous Routine] [Next Routine] [List of Routines]

     t04s_test

     Purpose: A few tests to verify that the model and the wrapper
     procedures work correctly

     $LastChangedBy: lphilpott $
     $LastChangedDate: 2012-06-14 11:16:07 -0700 (Thu, 14 Jun 2012) $
     $LastChangedRevision: 10562 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/external/IDL_GEOPACK/t04s/t04s_test.pro $

(See external/IDL_GEOPACK/t04s/t04s_test.pro)

## TT04S

[Previous Routine] [List of Routines]

    Procedure: tt04s

    Purpose:  tplot wrapper for the functional interface to the IDL Geopack
              implementation of the Tsyganenko-Sitnov (2004) storm-time geomagnetic field model.

    Input:
              pos_gsm_tvar: the tplot variable storing the position in
                  gsm coordinates

    Keywords:
              pdyn(optional): Solar wind pressure(nanoPascals) should either be a
                  string naming a tplot variable or an array or a single
                  value. If a tplot input is used it will be interpolated to
                  match the time inputs from the position var. Non-tplot array values
                  must match the number of times in the tplot input for pos_gsm_tvar

              dsti(optional): DST index(nanoTeslas)  should either be a
                  string naming a tplot variable or an array or a single
                  value.  If a tplot input is used it will be interpolated to
                  match the time inputs from the position var. Non-tplot array values
                  must match the number of times in the tplot input for pos_gsm_tvar

             yimf(optional): y component of the interplanetary magnetic field
                 should either be a string naming a tplot variable or an
                 array or a single value.  If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar

             zimf(optional): z component of the interplanetary magnetic field
                 should either be a string naming a tplot variable or an
                 array or a single value.  If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar

             w1(optional):  time integral from the beginning of a storm
                 can be an array or a tplot variable(see paper reference
                 below for definitions of w1-w6) or a single value.
                 If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar

             w2(optional): time integral from the beginning of a storm
                 can be an array or a tplot variable or a single value
                 If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar

             w3(optional):  time integral from the beginning of a storm
                 can be an array or a tplot variable or a single value
                 If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar

             w4(optional): time integral from the beginning of a storm
                 can be an array or a tplot variable or a single value
                 If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar

             w5(optional):  time integral from the beginning of a storm
                 can be an array or a tplot variable or a single value
                 If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar

             w6(optional): time integral from the beginning of a storm
                 can be an array or a tplot variable or a single value
                 If a tplot input is used it will
                 be interpolated to match the time inputs from the position
                 var. Non-tplot array values must match the number of times in the
                 tplot input for pos_gsm_tvar;

             parmod(optional): can input the Nx10 parmod array used by the
                 fortran Tsyganenko model instead of inputing parameters as
                 separate arrays. If passed as a raw array it will not be
                 modified or interpolated so be sure its has the correct
                 number of entries. It can also be passed as a tplot variable
                 name in which case it will be interpolated. If values are
                 passed individually and as par, the par values will be overwritten.

             period(optional): the amount of time between recalculations of
                 geodipole tilt in seconds(default: 60)  increase this
                 value to decrease run time

             get_nperiod(optional): Return the number of periods used in the time interval

             newname(optional):the name of the output variable.
                  (default: pos_gsm_tvar+'_bt04s') This option is ignored if
                  globbing is used.

             error(optional): named variable in which to return the
                  error state of this procedure call. 1 = success, 0 = failure

             get_tilt(optional):  Set this value to a tplot variable name in which the geodipole tilt for each period will be returned
                  One sample will be returned for each period with time at the center of the period.

             set_tilt(optional): Set this to a tplot variable name or an array of values containing the dipole tilt that should be used.
                  If a tplot input is used it will be interpolated to match the time inputs from the position
                  var. Non-tplot array values must match the number of times in the tplot input for pos_gsm_tvar
                  Notes:
                      1) set_tilt will cause add_tilt to be ignored
                      2) Due to this routine adding IGRF to the returned field, you cannot use set_tilt = 0 and give input
                          position values in SM coordinates; input position values are required to be in GSM coordinates due to the
                          IGRF calculation

             exact_tilt_times (optional):  Set this keyword to avoid grouping similar times (default 10 minutes) and instead
                  recalculate the dipole tilt at each input time

             add_tilt(optional): Set this to a tplot variable name or an array of values containing the values to be added to the dipole tilt
                  that should be used for each period. If a tplot input is used it will be interpolated to match the time inputs from the position
                  var. Non-tplot array values must match the number of times in the tplot input for pos_gsm_tvar

             geopack_2008 (optional): Set this keyword to use the latest version (2008) of the Geopack
                  library. Version 9.2 of the IDL Geopack DLM is required for this keyword to work.

             iopgen (optional): General option flag to pass to geopack_ts04. From Tsyganenko's Fortran:
                                      IOPGEN=0 - CALCULATE TOTAL FIELD
                                      IOPGEN=1 - DIPOLE SHIELDING ONLY
                                      IOPGEN=2 - TAIL FIELD ONLY
                                      IOPGEN=3 - BIRKELAND FIELD ONLY
                                      IOPGEN=4 - RING CURRENT FIELD ONLY
                                      IOPGEN=5 - INTERCONNECTION FIELD ONLY

             IOPT (optional)
             -  TAIL FIELD FLAG:       IOPT=0  -  BOTH MODES
                                       IOPT=1  -  MODE 1 ONLY
                                       IOPT=2  -  MODE 2 ONLY

             IOPB (optional)
             -  BIRKELAND FIELD FLAG: IOPB=0  -  ALL 4 TERMS
                                      IOPB=1  -  REGION 1, MODES 1 AND 2
                                      IOPB=2  -  REGION 2, MODES 1 AND 2

             IOPR (optional)
             -  RING CURRENT FLAG:    IOPR=0  -  BOTH SRC AND PRC
                                      IOPR=1  -  SRC ONLY
                                      IOPR=2  -  PRC ONLY

     Output: Stores the result of the field model calculations in tplot variables

     Notes:
            1. converts from normal gsm to rgsm by dividing vectors by earth's
                radius(6371.2 km) ie inputs should be in km
                6371.2 = the value used in the GEOPACK FORTRAN code for Re
            2. Input must be in GSM coordinates
            3. Haje Korth's IDL/Geopack DLM must be installed for this
                procedure to work
            4. either the variables setting parmod or the variables
                setting the individual parameter arrays should be set because
                the defaults aren't scientifically accurate
            5. model parameters that are input as tplot variables they
                will be interpolated to match the time values on the input
                position
            6.Find more documentation on the inner workings of the model,
                any gotchas, and the meaning of the arguments at:
                http://geo.phys.spbu.ru/~tsyganenko/modeling.html
                -or-
                http://ampere.jhuapl.edu/code/idl_geopack.html
            7. Definition of W1-W6 can be found at:
                N. A. Tsyganenko and M. I. Sitnov, Modeling the dynamics of the
                inner magnetosphere during strong geomagnetic storms, J. Geophys.
                Res., v. 110 (A3), A03208, doi: 10.1029/2004JA010798, 2005

     $LastChangedBy: nikos $
     $LastChangedDate: 2022-08-18 09:29:42 -0700 (Thu, 18 Aug 2022) $
     $LastChangedRevision: 31020 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/external/IDL_GEOPACK/t04s/tt04s.pro $

(See external/IDL_GEOPACK/t04s/tt04s.pro)