This page was created by the IDL library routine `mk_html_help2`.

Last modified: Wed Nov 5 03:16:59 2025.

# Directory Listing of Routines

# projects/iugonet/tools

- GET_PULSECODE_EISCAT
- IUG_GMAG_WDC_XYZ
  Transformation of geomagnetic field into XYZ (geographical) coordinates.

# Routine Descriptions

## GET_PULSECODE_EISCAT

[Next Routine] [List of Routines]

     FUNCTION: GET_PULSECODE_EISCAT
        pulse_out = get_pulsecode_eiscat(pulse_in, mode)

     :DESCRIPTION:
        Convert pulse_code_id of the EISCAT radar observation to
            pulse_code or vice versa.

     :KEYWORDS:
        pulse_in:  pulse_code_id(integer) or pulse_code(string)
        mode:      0(default) :     id     ---> pulse_code
                   others     : pulse_code --->     id
        pulse_out: output (pulse_code or id)

     Written by Y.-M. Tanaka, June 15, 2012 (ytanaka at nipr.ac.jp)

(See projects/iugonet/tools/get_pulsecode_eiscat.pro)

## IUG_GMAG_WDC_XYZ

[Previous Routine] [List of Routines]

    NAME:
    iug_gmag_wdc_xyz

    PURPOSE:
      Transformation of geomagnetic field into XYZ (geographical) coordinates.
      X:North, Y:East, Z:Vertical (downward is positive)

    SYNTAX:
      iug_gmag_wdc_xyz [ ,SITE = string ]

    KEYWORDS:
      site  = Station ABB code or name of geomagnetic index.
              Ex1) iug_gmag_wdc_xyz, site = 'kak', ...
              Ex2) iug_gmag_wdc_xyz, site = ['gua', 'kak'], ...
      reolution = Time resolution of the data: 'min' or 'hour'.

    EXAMPLE:
       iug_gmag_wdc_xyz, site = 'kak',resolution='min'

    CODE:
    A. Shinbori, 28/11/2012.
    A. Shinbori, 30/11/2017.

    MODIFICATIONS:

    ACKNOWLEDGEMENT:
     $LastChangedBy: nikos $
     $LastChangedDate: 2018-08-01 11:03:38 -0700 (Wed, 01 Aug 2018) $
     $LastChangedRevision: 25538 $
     $URL $

(See projects/iugonet/tools/iug_gmag_wdc_xyz.pro)