This page was created by the IDL library routine `mk_html_help2`.

Last modified: Fri Nov 7 18:17:52 2025.

# Directory Listing of Routines

# projects/erg/ground/riometer

- ERG_LOAD_ISEE_BRIO
  Loads the broadbeam riometer data obtained from ISEE riometer network.

# Routine Descriptions

## ERG_LOAD_ISEE_BRIO

[List of Routines]

     PROCEDURE: ERG_LOAD_ISEE_BRIO

     PURPOSE:
       Loads the broadbeam riometer data obtained from ISEE riometer network.

     KEYWORDS:
       site  = Observatory name, example, iug_load_brio_nipr, site='syo',
               the default is 'all', i.e., load all available stations.
               This can be an array of strings, e.g., ['ath', 'hus']
               or a single string delimited by spaces, e.g., 'ath hus'.
               Available sites as of July, 2017 : ath, kap, gak, hus
       datatype = observation frequency in MHz for imaging riometer
               At present, '30' is only available for datatype.
       trange = (Optional) Time range of interest  (2 element array).
       /verbose: set to output some useful info
       /downloadonly: if set, then only download the data, do not load it
               into variables.
       /no_download: use only files which are online locally.

     EXAMPLE:
       erg_load_isee_brio, site='ath', $
                     trange=['2017-03-20/00:00:00','2017-03-21/00:00:00']

     HISTORY:
     2017-07-06: Initial release by Satoshi Kurita, ISEE, Nagoya U.(kurita at isee.nagoya-u.ac.jp)
                 with support from Yoshimasa Tanaka (NIPR)

     $LastChangedDate: 2019-03-17 21:51:57 -0700 (Sun, 17 Mar 2019) $
     $LastChangedRevision: 26838 $

(See projects/erg/ground/riometer/erg_load_isee_brio.pro)