This page was created by the IDL library routine `mk_html_help2`.

Last modified: Wed Aug 27 18:18:06 2025.

# Directory Listing of Routines

# projects/SPP/fields/crib

- PSP_FLD_EXAMPLES
- PSP_FLD_QUALITY_FLAG_EXAMPLES
- PSP_FLD_QUALITY_FLAG_FILTER_EXAMPLES
- PSP_FLD_VENUS_EXAMPLES
- SPP_EVA_WIND_EXAMPLES
- SPP_FLD_EXAMPLES

# Routine Descriptions

## PSP_FLD_EXAMPLES

[Next Routine] [List of Routines]

     $LastChangedBy: pulupalap $
     $LastChangedDate: 2020-09-14 11:28:02 -0700 (Mon, 14 Sep 2020) $
     $LastChangedRevision: 29153 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/fields/crib/psp_fld_examples.pro $

(See projects/SPP/fields/crib/psp_fld_examples.pro)

## PSP_FLD_QUALITY_FLAG_EXAMPLES

[Previous Routine] [Next Routine] [List of Routines]

     PROCEDURE:  PSP_FLD_QUALITY_FLAG_EXAMPLES

     PURPOSE:    Plot examples of FIELDS data with various quality flags active.

     KEYWORDS:

       qf_type:  Specifies a quality flag. The routine will load and plot an
                 example of FIELDS data where that quality flag is active.

                 Options:  'BIAS_SWP', 'THRUSTER', 'SCM_CAL',
                           'MAG_ROLL', 'MAG_CAL', 'SPC_EMODE',
                           'SLS_CAL', 'OFF_UMBRA', 'OVERVIEW', 'ALL'

                 The 'qf_type' options correspond to the quality flags
                 included in the FIELDS Level 2 CDF files, with the
                 exception of the 'OVERVIEW' and 'ALL' type.
                 'OVERVIEW' plots an overview of all quality flags over
                 two example orbits, and 'ALL' plots all examples in
                 sequence.

                 If qf_type is set to 'BIAS_SWP' then two plots are created,
                 one showing a bias sweep from Encounter 1 and one from
                 Encounter 2. The difference between Encounter 1 sweeps
                 and those from subsequent Encounters is described below.

      no_pause:  By default, the routine pauses after a plot is made, and
                 waits for a continue command at the IDL prompt. Setting
                 this keyword eliminates this pause.

     EXAMPLE:

       IDL> psp_fld_quality_flag_examples, 'THRUSTER'

     $LastChangedBy: pulupalap $
     $LastChangedDate: 2020-11-12 22:39:16 -0800 (Thu, 12 Nov 2020) $
     $LastChangedRevision: 29352 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/fields/crib/psp_fld_quality_flag_examples.pro $

(See projects/SPP/fields/crib/psp_fld_quality_flag_examples.pro)

## PSP_FLD_QUALITY_FLAG_FILTER_EXAMPLES

[Previous Routine] [Next Routine] [List of Routines]

    NAME: PSP_FLD_QUALITY_FLAG_FILTER_EXAMPLES

    DESCRIPTION:
       Crib sheet to demonstrate how to filter and plot select PSP FIELDS data
       products based on the set quality flag filters.

    CALLING SEQUENCE:
       .run psp_fld_quality_flag_filter_examples
         OR
       cut-and-paste relevant portions to the command prompt

    NOTES:
       FIELDS quality flag filtering currently supports the following tplot
       variables:
         *psp_fld_l2_mag_RTN
         *psp_fld_l2_mag_SC
         *psp_fld_l2_mag_RTN_1min
         *psp_fld_l2_mag_SC_1min
         *psp_fld_l2_mag_RTN_4_Sa_per_Cyc
         *psp_fld_l2_mag_SC_4_Sa_per_Cyc

    CREATED BY: Ayris Narock (ADNET/GSFC) 2020

     $LastChangedBy: anarock $
     $LastChangedDate: 2020-11-18 13:19:37 -0800 (Wed, 18 Nov 2020) $
     $LastChangedRevision: 29360 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/fields/crib/psp_fld_quality_flag_filter_examples.pro $

(See projects/SPP/fields/crib/psp_fld_quality_flag_filter_examples.pro)

## PSP_FLD_VENUS_EXAMPLES

[Previous Routine] [Next Routine] [List of Routines]

     $LastChangedBy: pulupalap $
     $LastChangedDate: 2022-02-01 16:35:26 -0800 (Tue, 01 Feb 2022) $
     $LastChangedRevision: 30553 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/fields/crib/psp_fld_venus_examples.pro $

(See projects/SPP/fields/crib/psp_fld_venus_examples.pro)

## SPP_EVA_WIND_EXAMPLES

[Previous Routine] [Next Routine] [List of Routines]

     Script for loading Wind data

     to be used as dummy variables for SPP EVA burst selection tool development

     $LastChangedBy: pulupa $
     $LastChangedDate: 2017-01-13 12:03:00 -0800 (Fri, 13 Jan 2017) $
     $LastChangedRevision: 22595 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/fields/crib/spp_eva_wind_examples.pro $

(See projects/SPP/fields/crib/spp_eva_wind_examples.pro)

## SPP_FLD_EXAMPLES

[Previous Routine] [List of Routines]

     $LastChangedBy: pulupalap $
     $LastChangedDate: 2020-09-14 11:28:02 -0700 (Mon, 14 Sep 2020) $
     $LastChangedRevision: 29153 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/fields/crib/spp_fld_examples.pro $

(See projects/SPP/fields/crib/spp_fld_examples.pro)