This page was created by the IDL library routine `mk_html_help2`.

Last modified: Tue Sep 2 18:17:29 2025.

# Directory Listing of Routines

# projects/SPP/sweap/SPAN/ion

- SPP_SPACECRAFT_VERTICES
- SPP_SPACECRAFT_VERTICES_PLOT
- SPP_SWP_SPI_CMN_L2VARARR
  Returns an array with common block variable names for the input
- SPP_SWP_SPI_CONFIG_FLIGHT_BACKGROUND
- SPP_SWP_SPI_CONFIG_FLIGHT_CALIBRATION
- SPP_SWP_SPI_CONFIG_FLIGHT_CRUISE
- SPP_SWP_SPI_CONFIG_FLIGHT_HIGH
- SPP_SWP_SPI_CONFIG_FLIGHT_HIGH_RATE_CRUISE_MOMENTS
- SPP_SWP_SPI_CONFIG_FLIGHT_HIGH_RATE_MOMENTS_V2
- SPP_SWP_SPI_CONFIG_FLIGHT_LOW
- SPP_SWP_SPI_CONFIG_FLIGHT_MOMENTS
- SPP_SWP_SPI_CONFIG_MODE
- SPP_SWP_SPI_CONFIG_SWEM_STATE
- SPP_SWP_SPI_FLIGHT_ANO
- SPP_SWP_SPI_FLIGHT_DAC
- SPP_SWP_SPI_FLIGHT_DEF
- SPP_SWP_SPI_FLIGHT_EFF
- SPP_SWP_SPI_FLIGHT_ELO
- SPP_SWP_SPI_FLIGHT_ESA
- SPP_SWP_SPI_FLIGHT_EVT
- SPP_SWP_SPI_FLIGHT_GEO
- SPP_SWP_SPI_FLIGHT_LOA
- SPP_SWP_SPI_FLIGHT_MAS[1]
- SPP_SWP_SPI_FLIGHT_MAS[2]
- SPP_SWP_SPI_FLIGHT_MAS[2]
- SPP_SWP_SPI_FLIGHT_MAS[3]
- SPP_SWP_SPI_FLIGHT_MAS[4]
- SPP_SWP_SPI_FLIGHT_MAS[5]
- SPP_SWP_SPI_FLIGHT_MAS[6]
- SPP_SWP_SPI_FLIGHT_MAS[7]
- SPP_SWP_SPI_FLIGHT_MEM
- SPP_SWP_SPI_FLIGHT_MRAM_MAP
- SPP_SWP_SPI_FLIGHT_NRG
- SPP_SWP_SPI_FLIGHT_PAR
- SPP_SWP_SPI_FLIGHT_PRD
- SPP_SWP_SPI_FLIGHT_SCI
- SPP_SWP_SPI_FLIGHT_TBL
- SPP_SWP_SPI_FLIGHT_TOF
- SPP_SWP_SPI_RATES_APDAT__DEFINE
- SPP_SWP_SPI_SNAP
- SPP_SWP_SPI_TOF_APDAT__DEFINE

# Routine Descriptions

## SPP_SPACECRAFT_VERTICES

[Next Routine] [List of Routines]

     FUNCTION:        SPP_SPACECRAFT_VERTICES

     PURPOSE:         Collection of Parker Solar Probe spacecraft/instrument vertices and
                      rotation matrices for the purpose of plotting a model in
                      IDL. Vertices are in units of [mm] and in MAVEN_SPACECRAFT
                      coordinates.

     INPUT:           None.

     OUTPUT:          Structure containing vertices and rotation matrices.

     KEYWORDS:

         PLOT_SC1:     Plot all Parker Solar Probe vertices and SWEAP instrument locations.

     CREATED BY:      Roberto Livi on 2020-04-23

     VERSION:
       $LastChangedBy:
       $LastChangedDate:
       $LastChangedRevision:
       $URL

(See projects/SPP/sweap/SPAN/ion/spp_spacecraft_vertices.pro)

## SPP_SPACECRAFT_VERTICES_PLOT

[Previous Routine] [Next Routine] [List of Routines]

     FUNCTION:        SPP_SPACECRAFT_VERTICES_PLOT

     PURPOSE:

     INPUT:

     OUTPUT:

     KEYWORDS:

         PLOT_SC1:

     CREATED BY:      Roberto Livi on 2021-11-06

     VERSION:
       $LastChangedBy:
       $LastChangedDate:
       $LastChangedRevision:
       $URL

(See projects/SPP/sweap/SPAN/ion/spp_spacecraft_vertices_plot.pro)

## SPP_SWP_SPI_CMN_L2VARARR

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
     spp_swp_spi_cmn_l2vararr
    PURPOSE:
     Returns an array with common block variable names for the input
     apid.
    CALLING SEQUENCE:
     vars = spp_swp_spi_cmn_l2vararr(apid)
    INPUT:
     apid = the app_id for the data type;
    OUTPUT:
     vars = a 3, N array with common block variable names for the input
     apid, with three columns, one is the common block name, the second is
     the name in the CDF file, the third is 'Y' or 'N' for record
     variance.
    HISTORY:
     16-sep-2018, rlivi, rlivi@berkeley.edu
    SVN Berkeley Information:
     $LastChangedBy: rlivi2 $
     $LastChangedDate: 2018-12-03 23:01:25 -0800 (Mon, 03 Dec 2018) $
     $LastChangedRevision: 26222 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_cmn_l2vararr.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_cmn_l2vararr.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_BACKGROUND

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 2

     SWEM State Configuration for SPAN-Ai

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 26842 $
     $LastChangedDate: 2019-03-17 22:56:35 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_background.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_background.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_CALIBRATION

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 6

     SWEM State Configuration for SPAN-Ai

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 26842 $
     $LastChangedDate: 2019-03-17 22:56:35 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_calibration.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_calibration.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_CRUISE

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 7

     SWEM State Configuration for SPAN-Ai

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 26842 $
     $LastChangedDate: 2019-03-17 22:56:35 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_cruise.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_cruise.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_HIGH

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 4

     SWEM State Configuration for SPAN-Ai

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 26842 $
     $LastChangedDate: 2019-03-17 22:56:35 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_high.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_high.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_HIGH_RATE_CRUISE_MOMENTS

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 9

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 31610 $
     $LastChangedDate: 2023-03-09 13:20:37 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_high_rate_cruise_moments.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_high_rate_cruise_moments.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_HIGH_RATE_MOMENTS_V2

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 10

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 31611 $
     $LastChangedDate: 2023-03-09 13:21:01 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_high_rate_moments_v2.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_high_rate_moments_v2.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_LOW

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 3

     SWEM State Configuration for SPAN-Ai

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 26842 $
     $LastChangedDate: 2019-03-17 22:56:35 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_low.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_low.pro)

## SPP_SWP_SPI_CONFIG_FLIGHT_MOMENTS

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 5

     SWEM State Configuration for SPAN-Ai

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 26842 $
     $LastChangedDate: 2019-03-17 22:56:35 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_moments.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_flight_moments.pro)

## SPP_SWP_SPI_CONFIG_MODE

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_CONFIG_MODE

     Keywords:

     TMode: The configuration to load
          Options:
             Mode = 0
               - Name: RESERVED
               - Rate: NA
             Mode = 1
               - Name: SWEM Startup State
               - Rate:   15 Bytes/s
             Mode = 2
               - Name: Flight Background
               - Rate:   42 Bytes/s
             Mode = 3
               - Name: Flight Low Telemetry
               - Rate:  278 Bytes/s
             Mode = 4
               - Name: Flight High Telemetry
               - Rate: 2326 Bytes/s
             Mode = 5
               - Name: Moments
               - Rate: 5044 Bytes/s
             Mode = 6
               - Name: Calibration
               - Rate: 5044 Bytes/s
             Mode = 7
               - Name: Cruise
               - Rate: XXXX Bytes/s
             Mode = 8
               - Name: High Rate Moments
               - Rate: XXXX Bytes/s
             Mode = 9
               - Name: High Rate Cruise Moments
               - Rate: XXXX Bytes/s
             Mode = A
               - Name: High Rate Moments v2
               - Rate: XXXX Bytes/s

     $LastChangedDate: 2023-03-09 13:19:03 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_mode.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_mode.pro)

## SPP_SWP_SPI_CONFIG_SWEM_STATE

[Previous Routine] [Next Routine] [List of Routines]

                  MODE 1

     SWEM State Configuration for SPAN-Ai

     User must define the following tables
     -------------------------------------
     Product i | Full     | Mass j
     Product i | Targeted | Mass j
     0 <= i <= 2
     0 <= j <= 3
     Total: 24 Products

     Table Options
     -------------
     1D - '16A' , '32E' , '08D'
     2D - '08Dx32E' , '08Dx16A'
     3D - '08Dx32Ex16A'
     D - Deflector
     E - Energy
     A - Anode

     Special Case: '1D'
     ------------------
     This simply sums over all steps
     and anodes but leaves the mass
     variable.

     Summing Options
     ---------------
     Define exponent n of 2**n for
     Archive and Survey Products.
     ar - Archive
     sr - Survey
     Value range: 0 <= n <= 16

     SVN Properties
     --------------
     $LastChangedRevision: 26842 $
     $LastChangedDate: 2019-03-17 22:56:35 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_swem_state.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_config_swem_state.pro)

## SPP_SWP_SPI_FLIGHT_ANO

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_ANO

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 26433 $
     $LastChangedDate: 2019-01-06 22:10:25 -0800 (Sun, 06 Jan 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_ano.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_ano.pro)

## SPP_SWP_SPI_FLIGHT_DAC

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_DAC

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31605 $
     $LastChangedDate: 2023-03-09 13:12:04 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_dac.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_dac.pro)

## SPP_SWP_SPI_FLIGHT_DEF

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_DEF

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31605 $
     $LastChangedDate: 2023-03-09 13:12:04 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_def.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_def.pro)

## SPP_SWP_SPI_FLIGHT_EFF

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_EFF

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31612 $
     $LastChangedDate: 2023-03-09 13:22:18 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_eff.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_eff.pro)

## SPP_SWP_SPI_FLIGHT_ELO

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_ELO

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 28316 $
     $LastChangedDate: 2020-02-18 15:50:29 -0800 (Tue, 18 Feb 2020) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_elo.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_elo.pro)

## SPP_SWP_SPI_FLIGHT_ESA

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_ESA

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 26840 $
     $LastChangedDate: 2019-03-17 22:01:08 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_esa.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_esa.pro)

## SPP_SWP_SPI_FLIGHT_EVT

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_EVT

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31605 $
     $LastChangedDate: 2023-03-09 13:12:04 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_evt.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_evt.pro)

## SPP_SWP_SPI_FLIGHT_GEO

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_GEO

     Purpose:

     Taken from SWP_TN_011 SPAN Optics.pdf

     SVN Properties
     --------------
     $LastChangedRevision: 28314 $
     $LastChangedDate: 2020-02-18 15:49:41 -0800 (Tue, 18 Feb 2020) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_geo.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_geo.pro)

## SPP_SWP_SPI_FLIGHT_LOA

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_LOA

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31606 $
     $LastChangedDate: 2023-03-09 13:12:39 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_loa.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_loa.pro)

## SPP_SWP_SPI_FLIGHT_MAS[1]

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_MAS

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31606 $
     $LastChangedDate: 2023-03-09 13:12:39 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MAS[2]

[Previous Routine] [Next Routine] [List of Routines]

    ;#####################################################
    ;                  Mass Table 0
    ;#####################################################

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MAS[2]

[Previous Routine] [Next Routine] [List of Routines]

    ;#####################################################
    ;                  Mass Table 1
    ;#####################################################

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MAS[3]

[Previous Routine] [Next Routine] [List of Routines]

    ;#####################################################
    ;                  Mass Table 2
    ;#####################################################

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MAS[4]

[Previous Routine] [Next Routine] [List of Routines]

    ;#####################################################
    ;                  Mass Species
    ;#####################################################

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MAS[5]

[Previous Routine] [Next Routine] [List of Routines]

    ; Write to File

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MAS[6]

[Previous Routine] [Next Routine] [List of Routines]

    ; Mass Range LUT

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MAS[7]

[Previous Routine] [Next Routine] [List of Routines]

    ; Flight Mass Tables

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mas.pro)

## SPP_SWP_SPI_FLIGHT_MEM

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_MEM

     :Params:
        tables : in, optional, type=structure
           PSP SWEAP SPAN-Ai Flight MRAM Memory Map.
        config : in, optional, type=structure
           PSP SWEAP SPAN-Ai Flight Instrument Configuration

     SVN Properties
     --------------
     $LastChangedBy: rlivi04 $
     $LastChangedDate: 2023-03-09 13:12:39 -0800 (Thu, 09 Mar 2023) $
     $LastChangedRevision: 31606 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mem.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mem.pro)

## SPP_SWP_SPI_FLIGHT_MRAM_MAP

[Previous Routine] [Next Routine] [List of Routines]

     spp_swp_spi_flight_mram_map

     :Params:
        tables : in, optional, type=structure
           PSP SWEAP SPAN-Ai Flight MRAM Memory Map.
        config : in, optional, type=structure
           PSP SWEAP SPAN-Ai Flight Instrument Configuration
     $LastChangedBy: rlivi04 $
     $LastChangedDate: 2023-03-09 13:13:18 -0800 (Thu, 09 Mar 2023) $
     $LastChangedRevision: 31607 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mram_map.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_mram_map.pro)

## SPP_SWP_SPI_FLIGHT_NRG

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_NRG

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 26429 $
     $LastChangedDate: 2019-01-06 22:06:59 -0800 (Sun, 06 Jan 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_nrg.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_nrg.pro)

## SPP_SWP_SPI_FLIGHT_PAR

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_PAR

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31607 $
     $LastChangedDate: 2023-03-09 13:13:18 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_par.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_par.pro)

## SPP_SWP_SPI_FLIGHT_PRD

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_PRD

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 28310 $
     $LastChangedDate: 2020-02-18 15:48:09 -0800 (Tue, 18 Feb 2020) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_prd.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_prd.pro)

## SPP_SWP_SPI_FLIGHT_SCI

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_SCI

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 28315 $
     $LastChangedDate: 2020-02-18 15:49:56 -0800 (Tue, 18 Feb 2020) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_sci.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_sci.pro)

## SPP_SWP_SPI_FLIGHT_TBL

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_TBL

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 31607 $
     $LastChangedDate: 2023-03-09 13:13:18 -0800 (Thu, 09 Mar 2023) $
     $LastChangedBy: rlivi04 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_tbl.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_tbl.pro)

## SPP_SWP_SPI_FLIGHT_TOF

[Previous Routine] [Next Routine] [List of Routines]

     SPP_SWP_SPI_FLIGHT_TOF

     Purpose:

     SVN Properties
     --------------
     $LastChangedRevision: 26843 $
     $LastChangedDate: 2019-03-17 23:52:06 -0700 (Sun, 17 Mar 2019) $
     $LastChangedBy: rlivi2 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_tof.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_flight_tof.pro)

## SPP_SWP_SPI_RATES_APDAT__DEFINE

[Previous Routine] [Next Routine] [List of Routines]

     $LastChangedBy: davin-mac $
     $LastChangedDate: 2022-07-28 14:00:00 -0700 (Thu, 28 Jul 2022) $
     $LastChangedRevision: 30974 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_rates_apdat__define.pro $

     SPP_SWP_SPI_RATES_APDAT

     APID: 0x3BB
     Descritpion: SPAN-Ai Rates Package
     Size: 112 Bytes

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_rates_apdat__define.pro)

## SPP_SWP_SPI_SNAP

[Previous Routine] [Next Routine] [List of Routines]

     Ali 20190601
     $LastChangedBy: ali $
     $LastChangedDate: 2021-05-30 19:39:00 -0700 (Sun, 30 May 2021) $
     $LastChangedRevision: 30005 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_snap.pro $

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_snap.pro)

## SPP_SWP_SPI_TOF_APDAT__DEFINE

[Previous Routine] [List of Routines]

     $LastChangedBy: ali $
     $LastChangedDate: 2021-06-14 10:41:21 -0700 (Mon, 14 Jun 2021) $
     $LastChangedRevision: 30043 $
     $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/projects/SPP/sweap/SPAN/ion/spp_swp_spi_tof_apdat__define.pro $

     SPP_SWP_SPI_TOF_APDAT

     APID: 0x3BA
     Descritpion: SPAN-Ai TOF512 Package
     Size: 536 Bytes

(See projects/SPP/sweap/SPAN/ion/spp_swp_spi_tof_apdat__define.pro)