This page was created by the IDL library routine `mk_html_help2`.

Last modified: Fri Oct 3 18:17:41 2025.

# Directory Listing of Routines

# spedas_gui/panels/dproc

- SPD_UI_CLEAN_SPIKES_OPTIONS
  Front end interface allowing the user to select options for cleaning spikes from data.
- SPD_UI_CLIP_DATA_OPTIONS
  Front end interface allowing the user to select options for clipping data.
- SPD_UI_DEFLAG_OPTIONS
  Front end interface allowing the user to select options for deflagging data.
- SPD_UI_DEGAP_OPTIONS
  Front end interface allowing the user to select options for degapping data.
- SPD_UI_HIGH_PASS_OPTIONS
  Front end interface allowing the user to select high pass filter options.
- SPD_UI_INTERPOL_OPTIONS
  Front end window allowing user to select options for interpolation.
- SPD_UI_JOIN_VARIABLES_OPTIONS
  Front end interface allowing the user to select options for joining separate variables.
- SPD_UI_PWRSPC_OPTIONS
  A widget used to set keyword options for creating power spectra. This
- SPD_UI_SMOOTH_DATA_OPTIONS
  Front end interface allowing the user to select options for smoothing data.
- SPD_UI_TIME_DERIVATIVE_OPTIONS
  Front end interface allowing the user to select options for performing time derivatives on data.
- SPD_UI_WAVELET_OPTIONS
  A widget used to set keyword options for creating power spectra. This

# Routine Descriptions

## SPD_UI_CLEAN_SPIKES_OPTIONS

[Next Routine] [List of Routines]

    NAME:
      spd_ui_clean_spikes_options

    PURPOSE:
      Front end interface allowing the user to select options for cleaning spikes from data.

    CALLING SEQUENCE:
      return_values = spd_ui_clean_spikes_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       thresh: Threshold for determining spikes (see clean_spikes.pro)
       swidth: Width of smoothing window, see IDL documentation on smooth() for more info
       suffix: Suffix for new variable
       ok: Flag indicating success
      }

    $LastChangedBy:  $
    $LastChangedDate:  $
    $LastChangedRevision:  $
    $URL:  $

(See spedas_gui/panels/dproc/spd_ui_clean_spikes_options.pro)

## SPD_UI_CLIP_DATA_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_clip_data_options

    PURPOSE:
      Front end interface allowing the user to select options for clipping data.

    CALLING SEQUENCE:
      return_values = spd_ui_clip_data_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       maxc: maximum value for clipping
       minc: minimum value for clipping
       opts: Array of flags determining extra options
             [clip adjacent points, insert user-specified flag (instead of NaNs)]
       flag: user-specified flag, a double to be insterted where values are clipped
       suffix: Suffix for new variable
       ok: Flag indicating success
      }

    NOTES:

    $LastChangedBy:  $
    $LastChangedDate:  $
    $LastChangedRevision:  $
    $URL:  $

(See spedas_gui/panels/dproc/spd_ui_clip_data_options.pro)

## SPD_UI_DEFLAG_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_deflag_options

    PURPOSE:
      Front end interface allowing the user to select options for deflagging data.

    CALLING SEQUENCE:
      return_values = spd_ui_deflag_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       method: Array of flags specifying deflagging method
               [repeat last value, interpolate(linear), replace with value]
       opts: Array of flags determining extra options
             [set flag (default is 6.8792e28), set max gap size]
       flag: user-specified flag, will be removed in addition to NaNs & infinity
       maxgap: maximum gap size, in # of points, to be removed
       fillval: fill value, for replace option
       suffix: Suffix for new variable
       ok: Flag indicating success
      }

    NOTES:

    $LastChangedBy: $
    $LastChangedDate: $
    $LastChangedRevision: $
    $URL: $

(See spedas_gui/panels/dproc/spd_ui_deflag_options.pro)

## SPD_UI_DEGAP_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_degap_options

    PURPOSE:
      Front end interface allowing the user to select options for degapping data.

    CALLING SEQUENCE:
      return_values = spd_ui_degap_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       dt: Interval passed to degap routine
       margin: degap margin
       opts: Array of flags determining extra options
             [set degap flag, set max gap size]
       flag: User-specified flag to fill gaps with, uses NaNs if not set
       maxgap: Maximum gap size to be removed, uses total range of data if not set
       suffix: Suffix for new variable
       ok: Flag indicating success
      }

    NOTES:
      (Gaps are removed were greater than dt+margin and less than maxgap)

    $LastChangedBy:  $
    $LastChangedDate:  $
    $LastChangedRevision:  $
    $URL:  $

(See spedas_gui/panels/dproc/spd_ui_degap_options.pro)

## SPD_UI_HIGH_PASS_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_high_pass_options

    PURPOSE:
      Front end interface allowing the user to select high pass filter options.

    CALLING SEQUENCE:
      return_values = spd_ui_high_pass_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       dt: Time Resolution for smoothing
       icad: Interpolation cadence (not used by default)
       setICad: Flag to use interpolation cadence
       suffix: Suffix for new variable
       ok: Flag indicating success
      }

    NOTES:
      Options for the high pass filter are only used by smooth_in_time.pro to get
      the running average for calculation.  Since the call to smooth_in_time
      contains specific keywords some smoothing options are not available.

    $LastChangedBy:  $
    $LastChangedDate:  $
    $LastChangedRevision:  $
    $URL:  $

(See spedas_gui/panels/dproc/spd_ui_high_pass_options.pro)

## SPD_UI_INTERPOL_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_interpol_options

    PURPOSE:
      Front end window allowing user to select options for interpolation.

    CALLING SEQUENCE:
      result = spd_ui_interpol_options(gui_ID, historywin, statusbar, datap)

    INPUT:
      gui_id: group leader widget
      historywin: history window object
      statusbar: status bar object
      datap: pointer to loaded data object
      ptree: pointer to tree copy

    OUTPUT:
      values = {num, type, matchto, extrap, suffix, ok}
        num: number of points passed to interpol function
        type: type on interpolation (0=linear, 1=quad, 2=lst sqr qd, 3=spline, 4= nearest neighbor)
        matchto: pointer to copy of returned struct from loaded data obj,
                 specifies the selected quantity to match, null string if
                 none selected
        extrap: type of extrapolation for matching (0=none, 1=nan)
        suffix: optional suffix for new data quantity
        ok: flag indicating whether to procede with interpolation

    NOTES:

    $LastChangedBy: jwl $
    $LastChangedDate: 2022-02-25 13:27:50 -0800 (Fri, 25 Feb 2022) $
    $LastChangedRevision: 30620 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/spedas_gui/panels/dproc/spd_ui_interpol_options.pro $

(See spedas_gui/panels/dproc/spd_ui_interpol_options.pro)

## SPD_UI_JOIN_VARIABLES_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_join_variables_options

    PURPOSE:
      Front end interface allowing the user to select options for joining separate variables.

    CALLING SEQUENCE:
      return_values = spd_ui_join_variables_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       new_name: new_name for new variable
       ok: Flag indicating success
      }

    NOTES:

    $LastChangedBy: jwl $
    $LastChangedDate: 2022-02-25 13:27:50 -0800 (Fri, 25 Feb 2022) $
    $LastChangedRevision: 30620 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/spedas_gui/panels/dproc/spd_ui_join_variables_options.pro $

(See spedas_gui/panels/dproc/spd_ui_join_variables_options.pro)

## SPD_UI_PWRSPC_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_pwrspc_options

    PURPOSE:
      A widget used to set keyword options for creating power spectra.  This
      widget returns an anonymous structure of keyword settings that is passed
      through the OPTIONS positional parameter of SPD_UI_PWRSPC.  Intended to
      be called from SPD_UI_DPROC.

    CALLING SEQUENCE:
      opt_struct = spd_ui_pwrspc_options(gui_id, trObj, historyWin, statusBar)

    INPUT:
      gui_id: The GUI id that should be the top level id of the Data Processing
              window.
      trObj: The timerange object that is created in SPD_GUI.
      historyWin: The history window object.
      statusBar: The status bar object for the Data Processing window.

    KEYWORDS:
      none

    OUTPUT:
      opt_struct: The anonymous structure contain options and keyword settings for
                  SPD_UI_PWRSPC.

    $LastChangedBy: jwl $
    $LastChangedDate: 2022-02-25 13:27:50 -0800 (Fri, 25 Feb 2022) $
    $LastChangedRevision: 30620 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/spedas_gui/panels/dproc/spd_ui_pwrspc_options.pro $

(See spedas_gui/panels/dproc/spd_ui_pwrspc_options.pro)

## SPD_UI_SMOOTH_DATA_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_smooth_data_options

    PURPOSE:
      Front end interface allowing the user to select options for smoothing data.

    CALLING SEQUENCE:
      return_values = spd_ui_smooth_data_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       dt: Time Resolution for smoothing
       icad: Interpolation cadence (not used by default)
       setICad: Flag to use interpolation cadence
       dttype: Array of flags determining how smoothing is applied [default,forward,backward]
       opts: Array of flags determining extra options [no_time_intrp,true_t_integtration,smooth_nans]
       suffix: Suffix for new variable
       ok: Flag indicating success
      }

    NOTES:

    $LastChangedBy:  $
    $LastChangedDate:  $
    $LastChangedRevision:  $
    $URL:  $

(See spedas_gui/panels/dproc/spd_ui_smooth_data_options.pro)

## SPD_UI_TIME_DERIVATIVE_OPTIONS

[Previous Routine] [Next Routine] [List of Routines]

    NAME:
      spd_ui_time_derivative_options

    PURPOSE:
      Front end interface allowing the user to select options for performing time derivatives on data.

    CALLING SEQUENCE:
      return_values = spd_ui_time_derivative_options(gui_id, statusbar, historywindow)

    INPUT:
      gui_id: widget id of group leader
      statusbar: status bar object ref.
      historywindow: history window object ref.

    OUTPUT:
      return values: anonymous structure containing input parameters for dproc routine
      {
       swidth: Width of smoothing window, see IDL documentation on smooth() for more info
       setswidth: Flag indicating whether data is to be smoothed
       suffix: Suffix for new variable
       ok: Flag indicating success
      }

    NOTES:

    $LastChangedBy:  $
    $LastChangedDate:  $
    $LastChangedRevision:  $
    $URL:  $

(See spedas_gui/panels/dproc/spd_ui_time_derivative_options.pro)

## SPD_UI_WAVELET_OPTIONS

[Previous Routine] [List of Routines]

    NAME:
      spd_ui_wavelet_options

    PURPOSE:
      A widget used to set keyword options for creating power spectra.  This
      widget returns an anonymous structure of keyword settings that is passed
      through the OPTIONS positional parameter of SPD_UI_WAVELET.  Intended to
      be called from SPD_UI_DPROC.

    CALLING SEQUENCE:
      opt_struct = spd_ui_wavelet_options(gui_id, trObj, historyWin,
                   statusBar, varname)

    INPUT:
      gui_id: The GUI id that should be the top level id of the Data Processing
              window.
      dataobj: The data object
      trObj: The timerange object that is created in SPD_GUI.
      historyWin: The history window object.
      statusBar: The status bar object for the Data Processing window.
      varname: The variable name -- since wavlet defaults depend on the
               time resoultion of each variable, this need to be done
               separately for each one
    KEYWORDS:
      none

    OUTPUT:
      opt_struct: The anonymous structure contain options and keyword settings for
                  SPD_UI_WAVELET.

    $LastChangedBy: jwl $
    $LastChangedDate: 2022-02-25 13:27:50 -0800 (Fri, 25 Feb 2022) $
    $LastChangedRevision: 30620 $
    $URL: svn+ssh://thmsvn@ambrosia.ssl.berkeley.edu/repos/spdsoft/trunk/spedas_gui/panels/dproc/spd_ui_wavelet_options.pro $

(See spedas_gui/panels/dproc/spd_ui_wavelet_options.pro)